{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":6,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RXM-A9"]
[]
[]
[]
[]
["","","","","FCAG35BVEB / RXM35A5V1B9","FCAG50BVEB / RXM50A5V1B9"]
["Totale koelcapaciteit","Nom.","","kW","3.5","5"]
["Totale verwarmingscapaciteit","Nom.","","kW","4.2","6"]
["Nominaal rendement","EER","","","3.72","3.58"]
["","COP","","","3.77","3.7"]
["","Jaarlijks energieverbruik","","kWu","470","698"]
["Nominaal energierendement","Richtlijn Energielabels","Koeling","","A","A"]
["","","Verwarming","","A","A"]
["Koeling","Koeling-=-Energieklasse","","","A++","A++"]
["","Vermogen","Pdesign","kW","3.5","5"]
["","SEER","","","6.51","6.54"]
["","Jaarlijks energieverbruik","","kWu/a","188","268"]
["Verwarming (gematigd klimaat)","Energieklasse","","","A++","A+"]
["","Vermogen","Pdesign","kW","3.32","4.36"]
["","SCOP/A","","","4.98","4.3"]
["","Pdh-verwarmingsvermogen bij -10 °C","","kW","2.67","3.86"]
["","Jaarlijks energieverbruik","","kWu/a","933","1418"]
["Bereik van het energierendement","","","","A+++ ~ D","A+++ ~ D"]
["Opmerkingen","","","","(1) - Zie afzonderlijke afbeelding voor bedrijfsbereik","(1) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemp.: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m."]
["","","","","(2) - Voor elektrische gegevens zie afzonderlijke tekening","(2) - Nominale verwarmingscapaciteiten gebaseerd op: binnentemperatuur: 20°CDB, buitentemperatuur: 7°CDB/6°CWB, equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0m."]
["","","","","(3) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemp.: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m.","(3) - Zie afzonderlijke afbeelding voor bedrijfsbereik"]
["","","","","(4) - Nominale verwarmingscapaciteiten gebaseerd op: binnentemperatuur: 20°CDB, buitentemperatuur: 7°CDB/6°CWB, equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0m.","(4) - Voor elektrische gegevens zie afzonderlijke tekening"]