{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":5,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RXM-R9"]
[]
[]
[]
[]
["","","","","FCAG35BVEB / RXM35R5V1B9"]
["Koelcapaciteit","Nom.","","kW","3.50"]
["Totale verwarmingscapaciteit","Nom.","","kW","4.20"]
["Nominaal energierendement","EER","","","3.72"]
["","COP","","","3.77"]
["","Jaarlijks energieverbruik","","kWu","470"]
["","Richtlijn Energielabels","Koeling","","A"]
["","","Verwarming","","A"]
["Koeling","Energieklasse","","","A++"]
["","Vermogen","Pdesign","kW","3.50"]
["","SEER","","","6.35"]
["","Jaarlijks energieverbruik","","kWu/a","193"]
["Verwarming (gematigd klimaat)","Energieklasse","","","A++"]
["","Vermogen","Pdesign","kW","3.32"]
["","SCOP/A","","","4.90"]
["","Jaarlijks energieverbruik","","kWu/a","948"]
["Opmerkingen","","","","(1) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemperatuur: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m."]
["","","","","(2) - Nominale verwarmingscapaciteiten gebaseerd op: binnentemperatuur: 20°CDB, buitentemperatuur: 7°CDB/6°CWB, equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0m."]
["","","","","(3) - Zie afzonderlijke afbeelding voor bedrijfsbereik"]
["","","","","(4) - Voor elektrische gegevens zie afzonderlijke tekening"]