{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":10,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RZAG-B"]
[]
[]
[]
[]
["","","","","FCAG50BVEB / RZAG35B5V1B","FCAG35BVEB / RZAG35B5V1B","FCAG60BVEB / RZAG50B5V1B","FCAG50BVEB / RZAG50B5V1B","FCAG71BVEB / RZAG60B5V1B","FCAG60BVEB / RZAG60B5V1B"]
["Totale koelcapaciteit","Min.","","kW","1.6","1.6","1.7","1.7","1.7","1.7"]
["","Nom.","","kW","3.5","3.5","5","5","6","6"]
["","Max.","","kW","4.5","4.5","6","6","6.5","6.5"]
["Totale verwarmingscapaciteit","Min.","","kW","1.4","1.4","1.5","1.5","1.6","1.6"]
["","Nom.","","kW","4","4","5.8","5.8","7","7"]
["","Max.","","kW","5","5","6","6","7.5","7.5"]
["Nominaal rendement","EER","","","4.57","4.4","3.98","3.9","3.79","3.4"]
["","COP","","","4.41","4.3","3.75","3.71","3.53","3.4"]
["","Jaarlijks energieverbruik","","kWu","383","398","628","641","792","882"]
["Nominaal energierendement","Richtlijn Energielabels","Koeling","","A","A","A","A","A","A"]
["","","Verwarming","","A","A","A","A","B","C"]
["Koeling","Koeling-=-Energieklasse","","","A++","A++","A++","A++","A++","A++"]
["","Vermogen","Pdesign","kW","3.5","3.5","5","5","6","6"]
["","SEER","","","7.4","7.3","6.93","6.8","6.82","6.6"]
["","Jaarlijks energieverbruik","","kWu/a","166","168","252","257","308","318"]
["Verwarming (gematigd klimaat)","Energieklasse","","","A+","A+","A+","A+","A+","A+"]
["","Vermogen","Pdesign","kW","3.3","3.3","4.3","4.3","4.6","4.6"]
["","SCOP/A","","","4.41","4.3","4.35","4.3","4.39","4.25"]
["","Pdh-verwarmingsvermogen bij -10 °C","","kW","2.91","2.91","3.73","3.68","4","3.96"]
["","Jaarlijks energieverbruik","","kWu/a","1048","1074","1384","1398","1467","1515"]
["Bereik van het energierendement","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]