{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":61,"n_cols":8,"rows_kept":61,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-H"]
[]
[]
[]
[]
["","","","","","FCAHG100HVEB","FCAHG125HVEB","FCAHG140HVEB"]
["Totale koelcapaciteit","Totale capaciteit","","Nom.","kW","9.50","12.10","13.40"]
["Verwarmingscapaciteit","Totaalvermogen","","Nom.","kW","10.8","13.5","15.5"]
["Behuizing","Materiaal","","","","Gegalvaniseerde staalplaat","Gegalvaniseerde staalplaat","Gegalvaniseerde staalplaat"]
["Afmetingen","Unit","","Hoogte","mm","288","288","288"]
["","","","Breedte","mm","840","840","840"]
["","","","Diepte","mm","840","840","840"]
["Gewicht","Unit","","","kg","25","25","25"]
["Ventilator-","Luchthoeveelheid","Koelen","Hoog","m³/min","32.2","34.4","34.4"]
["Ventilator","Luchtdebiet","Koeling","Middelhoog","m³/min","25.7","27.3","27.3"]
["Ventilator-","Luchthoeveelheid","Koelen","Laag","m³/min","19.1","21.2","21.2"]
["","","Verwarmen","Hoog","m³/min","30.8","32.1","32.1"]
["Ventilator","Luchtdebiet","Verwarming","Middelhoog","m³/min","24.6","25.5","25.5"]
["Ventilator-","Luchthoeveelheid","Verwarmen","Laag","m³/min","18.3","19.7","19.7"]
["Geluidsvermogenniveau","Koelen","","","dB(A)","61","61","61"]
["","Verwarmen","","","dB(A)","61","61","61"]
["Geluidsdrukniveau op 1 m","Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Hoog-=-dB(A)","dB(A)","44","45","45"]
["Geluidsdrukniveau","Koeling","","Middelhoog","dB(A)","39","40","41"]
["Geluidsdrukniveau op 1 m","Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Laag-=-dB(A)","dB(A)","33","35","37"]
["","Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Hoog-=-dB(A)","dB(A)","44","45","45"]
["Geluidsdrukniveau","Verwarming","","Middelhoog","dB(A)","39","40","41"]
["Geluidsdrukniveau op 1 m","Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Laag-=-dB(A)","dB(A)","33","35","37"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","9.52","9.52","9.52"]
["","Gas","","Buitendiameter","mm","15.9","15.9","15.9"]
["","Drainage","","","","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)"]
["Sierpaneel","Model","","","","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B"]
["","Afmetingen","","Hoogte","mm","65","65","65"]
["","","","Breedte","mm","950","950","950"]
["","","","Diepte","mm","950","950","950"]
["","Gewicht","","","kg","5.5","5.5","5.5"]
["Sierpaneel 2","Model","","","","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B"]
["","Afmetingen","","Hoogte","mm","148","148","148"]
["","","","Breedte","mm","950","950","950"]
["","","","Diepte","mm","950","950","950"]
["","Gewicht","","","kg","10.3","10.3","10.3"]
["Sierpaneel 3","Model","","","","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB"]
["","Afmetingen","","Hoogte","mm","106","106","106"]
["","","","Breedte","mm","950","950","950"]
["","","","Diepte","mm","950","950","950"]
["","Gewicht","","","kg","6.5","6.5","6.5"]
["Regelsystemen","Infrared remote control","","","","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB"]
["Regelsystemen","Bedrade afstandsbediening","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Standaard-accessoires","Installation manual","","","","1","1","1"]
["","Washer for hanger bracket","","","","8","8","8"]
["","Operation manual","","","","1","1","1"]
["","Wire clamp material","","","","7","7","7"]
["","Clamp for drain hose","","","","1","1","1"]
["","Clamps","","","","1","1","1"]
["","Drain hose","","","","1","1","1"]
["","Installation guide","","","","1","1","1"]
["","Insulation for fitting","","","","2","2","2"]
["","Screws","","","","4","4","4"]
["","Sealing pads","","","","1","1","1"]
["Voeding","Fase","","","","1~","1~","1~"]
["Spanningsvorm","Spanningsvorm-=-Frequentie","","Frequentie","","50/60","50/60","50/60"]
["","Spanningsvorm-=-Spanning","","Spanning","","220-240/220","220-240/220","220-240/220"]