{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":22,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / RZQSG-LV1/LY1"]
[]
[]
[]
[]
["","","","","FCQG35FVEB / FCQG35FVEB / RZQSG71L2V1B","FCQG71FVEB / RZQSG71L2V1B","FCQG100FVEB / RZQSG100L7V1B","FCQG100FVEB / RZQSG100L7Y1B","FCQG50FVEB / FCQG50FVEB / RZQSG100L7V1B","FCQG100FVEB / RZQSG100L7Y1B9","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQSG100L7V1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQSG100L7Y1B9","FCQG50FVEB / FCQG50FVEB / RZQSG100L7Y1B9","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQSG125L7V1B","FCQG50FVEB / FCQG50FVEB / FCQG50FVEB / RZQSG125L7V1B","FCQG60FVEB / FCQG60FVEB / RZQSG125L7V1B","FCQG125FVEB / RZQSG125L7V1B","FCQG125FVEB / RZQSG125L7Y1B9","FCQG125FVEB / RZQSG125L7Y1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQSG125L7Y1B9","FCQG50FVEB / FCQG50FVEB / FCQG50FVEB / RZQSG125L7Y1B9","FCQG60FVEB / FCQG60FVEB / RZQSG125L7Y1B9"]
["Totale koelcapaciteit","Nom.","","kW","","6.8","9.5","9.5 (3)","","9.5","","","","","","","12.0","12.0","12.0 (3)"]
["Koeling","SEER","","","4.30","5.11","5.11","5.11 (6)","4.30","5.11","4.30","4.30","4.30","4.00","4.30","4.30","5.11","5.11","5.11 (6)","4.00","4.30","4.30"]
["","Jaarlijks energieverbruik","","kWu/a","554","466","650.685","","773.256","650.685","773.256","773.256","773.256","1,050","976.744","976.744","821.918","821.918","","1,050","976.744","976.744"]
["","Vermogen","Pdesign","kW","6.80","6.80","9.50","","9.50","9.50","9.50","9.50","9.50","12.00","12.00","12.00","12.00","12.00","","12.00","12.00","12.00"]
["","Energieklasse","","","C","A","A","","C","A","C","C","C","D","C","C","A","A","","D","C","C"]
["Verwarming (gematigd klimaat)","Vermogen","Pdesign","kW","6.00","6.33","7.60","","6.81","7.60","6.81","6.81","6.81","8.03","8.03","8.03","8.03","8.03","","8.03","8.03","8.03"]
["","SCOP/A","","","3.40","3.81","3.80","3.80 (6)","3.40","3.80","3.40","3.40","3.40","3.40","3.40","3.40","3.81","3.81","3.81 (6)","3.40","3.40","3.40"]
["","Energieklasse","","","A","A","A","","A","A","A","A","A","A","A","A","A","A","","A","A","A"]
["","Jaarlijks energieverbruik","","kWu/a","2,472","2,327","2,799","","2,802","2,799","2,802","2,802","2,802","3,305","3,305","3,306.471","2,949","2,949","","3,305","3,305","3,306.471"]
["Nominaal energierendement","Jaarlijks energieverbruik","","kWu","","971","1,440","1,440","","1,440","","","","","","","1,870","1,870","1,870"]
["","EER","","","","3.21","3.30","3.30","","3.30","","","","","","","3.21","3.21","3.21"]
["","COP","","","","3.61","3.54","3.54","","3.54","","","","","","","3.41","3.41","3.41"]
["","Richtlijn Energielabels","Koeling","","","A","A","A","","A","","","","","","","A","A","A"]
["","","Verwarming","","","A","B","A","","B","","","","","","","B","B","B"]
["Totale verwarmingscapaciteit","Nom.","","kW","","7.5","10.8","10.8 (4)","","10.8","","","","","","","13.5","13.5","13.5 (4)"]
["Opmerkingen","","","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","(1) - Jaarlijks energieverbruik: op basis van een gemiddelde van 500 bedrijfsuren per jaar bij vollast (nominale omstandigheden)","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","","","","","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","(1) - Jaarlijks energieverbruik: op basis van een gemiddelde van 500 bedrijfsuren per jaar bij vollast (nominale omstandigheden)"]
["","","","","","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting","(2) - Energielabel: schaalverdeling van A (meest efficiënt) tot G (minst efficiënt)","","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting","","","","","","","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting","(2) - Energielabel: schaalverdeling van A (meest efficiënt) tot G (minst efficiënt)"]
["","","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU"]
["","","","","","","","(3) - Koelen: binnentemp. 27°CDB, 19°CWB; buitentemperatuur. 35°CDB; equivalente leidinglengte: 5 m; hoogteverschil: 0m","","","","","","","","","","","(3) - Koelen: binnentemp. 27°CDB, 19°CWB; buitentemperatuur. 35°CDB; equivalente leidinglengte: 5 m; hoogteverschil: 0m"]
["","","","","","","","(4) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5 m; hoogteverschil: 0m","","","","","","","","","","","(4) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5 m; hoogteverschil: 0m"]
["","","","","","","","(5) - Jaarlijks energieverbruik is conform richtlijn 2002/31/EC inzake energielabels","","","","","","","","","","","(5) - Jaarlijks energieverbruik is conform richtlijn 2002/31/EC inzake energielabels"]
["","","","","","","","(6) - SEER en SCOP zijn conform EN 14825","","","","","","","","","","","(6) - SEER en SCOP zijn conform EN 14825"]
["","","","","","","","(7) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting","","","","","","","","","","","(7) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting"]