{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":13,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQHG-F / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCQHG100FVEB / RZQG71L8Y1B","FCQHG71FVEB / RZQG71L8Y1B","FCQHG100FVEB / RZQG100L8Y1B","FCQHG140FVEB / RZQG100L8Y1B","FCQHG71FVEB / FCQHG71FVEB / RZQG100L8Y1B","FCQHG125FVEB / RZQG125L8Y1B","FCQHG140FVEB / RZQG125L8Y1B","FCQHG71FVEB / FCQHG71FVEB / RZQG125L8Y1B","FCQHG140FVEB / RZQG140L7Y1B"]
["Totale koelcapaciteit","Nom.","","kW","","6.80","9.5","","","12.0","","","13.4"]
["Koeling","SEER","","","7.00","6.91","7","7.00","5.10","6.61","6.61","5.10"]
["","Jaarlijks energieverbruik","","kWu/a","340","345","475","475","652","636","636","824"]
["","Vermogen","Pdesign","kW","6.80","6.80","9.5","9.50","9.50","12","12.00","12.00"]
["","Energieklasse","","","A++","A++","A++","A++","B","A++","A++","B"]
["Verwarming (gematigd klimaat)","Vermogen","Pdesign","kW","7.60","7.60","11.3","11.30","11.30","12.66","12.66","12.71"]
["","SCOP/A","","","4.54","4.54","4.8","4.80","3.80","4.63","4.63","3.80"]
["","Energieklasse","","","A+","A+","A++","A++","A","A++","A++","A"]
["","Jaarlijks energieverbruik","","kWu/a","2,344","2,344","3,296","3,296","4,164","3,829","3,829","4,683"]
["Nominaal energierendement","Jaarlijks energieverbruik","","kWh","","830","1,075","","","1,500"]
["","EER","","","","4.09","4.42","","","4.00","","","3.35"]
["","COP","","","","4.80","4.99","","","4.40","","","4.12"]
["","Richtlijn Energielabels","Koeling","","","A","A","","","A"]
["","","Verwarming","","","A","A","","","A"]
["Totale verwarmingscapaciteit","Nom.","","kW","","7.5","10.8","","","13.5","","","15.5"]
["Opmerkingen","","","","","(1) - Jaarlijks energieverbruik is conform richtlijn 2002/31/EC inzake energielabels","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU"]
["","","","","","(2) - SEER en SCOP zijn conform EN 14825","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting","","","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting","","","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting"]