{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":67,"n_cols":8,"rows_kept":67,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDA-A"]
[]
[]
[]
[]
["","","","","","FDA125A5VEB","FDA200AXVEB","FDA250AXVEB"]
["Totale koelcapaciteit","Totale capaciteit","","Nom.","kW","12.10","19.00","22.00"]
["Totale verwarmingscapaciteit","Totaalvermogen","","Nom.","kW","13.50","22.4","24.0"]
["Behuizing","Kleur","","","","Ongelakt","Ongelakt","Ongelakt"]
["","Materiaal","","","","Gegalvaniseerd staal","Gegalvaniseerde staalplaat","Gegalvaniseerde staalplaat"]
["Afmetingen","Unit","","Hoogte","mm","300","470","470"]
["","","","Breedte","mm","1,400","1,490","1,490"]
["","","","Diepte","mm","700","1,100","1,100"]
["Gewicht","Unit","","","kg","45","104","115"]
["Vereiste plafondruimte >","mm","","","","350"]
["Ventilator","Luchthoeveelheid","Koelen","Hoog","m³/min","39.0","64.0","69.0"]
["","","","Middelhoog","m³/min","","50","56"]
["","","","Laag","m³/min","28.0","36.0","43.0"]
["","","Verwarmen","Hoog","m³/min","39.0","64.0","69.0"]
["","","","Middelhoog","m³/min","","50.0","56.0"]
["","","","Laag","m³/min","28.0","36.0","43.0"]
["","Externe statische druk","","Hoog","Pa","200","250","250"]
["","","","Nom.","Pa","50","62","62"]
["Geluidsvermogenniveau","Koelen","","","dBA","66","69.0","71.0"]
["Geluidsdrukniveau op 1 m","Koelen","","Hoog","dBA","40","43.0","44.0"]
["","","","Middelhoog","dBA","","39.0","40.0"]
["","","","Laag","dBA","33","36.0","37.0"]
["","Verwarmen","","Hoog","dBA","40","43.0","44.0"]
["","","","Middelhoog","dBA","","39.0","40.0"]
["","","","Laag","dBA","33","36.0","37.0"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","9.52","9.52","9.52"]
["","Gas","","Buitendiameter","mm","15.90","19.1","22.2"]
["","Afvoer","","","","VP25 (I.D. 25/O.D. 32)","BSP1","BSP1"]
["Afvoerhoogte","mm","","","","625"]
["Sierpaneel","Model","","","","BYBS125DJW1"]
["","Kleur","","","","Wit (10Y9/0.5)"]
["","Afmetingen","","Hoogte","mm","55"]
["","","","Breedte","mm","1,500"]
["","","","Diepte","mm","500"]
["","Gewicht","","","kg","6.5"]
["Regelsystemen","Infrared remote control","","","","BRC4C65, BRC4C66"]
["","Wired remote control","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Standaard-accessoires","Schroeven","","","","16","2","2"]
["","Sluitring","","","","8","12","12"]
["","Slangband","","","","1"]
["","Afvoerslang","","","","1"]
["","Algemene voorzorgsmaatregelen","","","","1","1","1"]
["","Montage- en bedieningshandleiding","","","","1","1","1"]
["","Draad voor gemeenschappelijke netvoeding","","","","2"]
["","Dichtingsmateriaal (aftapslang)","","","","1"]
["","Afdichtingsmateriaal","","","","2"]
["","Thermische isolatiebuis (vloeistof)","","","","1"]
["","Thermische isolatiebuis (gas)","","","","1"]
["Power supply","Naam","","","","","VE","VE"]
["","Fase","","","","1~","1~","1~"]
["","Frequentie","","","Hz","50/60","50/60","50/60"]
["","Spanning","","","V","220-240/220","220-240/220","220-240/220"]
["Opmerkingen","","","","","(1) - Voor elektrische gegevens zie afzonderlijke tekening"]
["Standaard-accessoires","Bedieningshandleiding","","","","","1","1"]
["","Montagehandleiding","","","","","1","1"]
["","Gasaansluitleiding","","","","","1","1"]
["","Draadklem","","","","","1","1"]
["","Veerring","","","","","2","2"]
["","Schroef + dichtingsring","","","","","45","45"]
["","Zeskantschroef met sluitring","","","","","49","49"]
["","Zeskantschroef","","","","","2","2"]
["","Vlakke sluitring","","","","","8","8"]