{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDBQ-B"]
[]
[]
[]
[]
["","","","","","FDBQ25B5V1","FDBQ25B8V1"]
["Geluidsdrukniveau op 1 m","Verwarmen","","Hoog","dBA","35.0","35.0"]
["","","","Laag","dBA","29.0","29.0"]
["","Koelen","","Laag","dBA","28.0","28.0"]
["","","","Hoog","dBA","35.0","35.0"]
["Standaard-accessoires","Montage- en bedieningshandleiding","","","","1","1"]
["","Aanzuigfilter","","","","1","1"]
["Regelsystemen","Wired remote control","","","","BRC1D52, BRC1E52A/B"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","6.35"]
["","Gas","","Buitendiameter","mm","9.52"]
["","Afvoer","","","","27.2"]
["Geluidsvermogenniveau","Koelen","","","dBA","55","55"]
["","Verwarmen","","","dBA","55","55"]
["Afmetingen","Unit","","Breedte","mm","652","652"]
["","","","Diepte","mm","502","502"]
["","","","Hoogte","mm","230","230"]
["Behuizing","Materiaal","","","","Verzinkt plaatstaal","Verzinkt plaatstaal"]
["Gewicht","Unit","","","kg","17.0","17.0"]
["Ventilator","Luchthoeveelheid","Verwarmen","Hoog","m³/min","","6.95"]
["","","","Laag","m³/min","","5.20"]
["","","Koelen","Laag","m³/min","","5.20"]
["","","","Hoog","m³/min","","6.50"]
["Power supply","Fase","","","","1~","1~"]
["","Frequentie","","","Hz","50","50"]
["","Naam","","","","V1","V1"]
["","Spanning","","","V","230","230 +/-10%"]
["Opmerkingen","","","","","(1) - De geluidswaarden worden in een semi-echoloze ruimte gemeten.","(1) - De geluidswaarden worden in een semi-echoloze ruimte gemeten."]
["","","","","","(2) - Het geluidsdrukniveau is een relatieve waarde, die afhankelijk is van de afstand en de akoestische omgeving. Zie de geluidsniveautekeningen voor meer bijzonderheden.","(2) - Het geluidsdrukniveau is een relatieve waarde, die afhankelijk is van de afstand en de akoestische omgeving. Zie de geluidsniveautekeningen voor meer bijzonderheden."]
["","","","","","(3) - Het geluidsvermogenniveau is een absolute waarde, die het door een geluidsbron gegenereerde vermogen aangeeft.","(3) - Het geluidsvermogenniveau is een absolute waarde, die het door een geluidsbron gegenereerde vermogen aangeeft."]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","","6.35"]
["","Gas","","Buitendiameter","mm","","9.52"]
["","Afvoer","","","","","27.2"]