{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":7,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-C / RZQSG-LV1/LY1"]
[]
[]
[]
[]
["","","","","FDQ125C7VEB / RZQSG125L7V1B","FDQ125C7VEB / RZQSG125L7Y1B9","FDQ125C7VEB / RZQSG125L7Y1B"]
["Totale koelcapaciteit","Nom.","","kW","12.0","12.0","12.0 (3)"]
["Koeling","SEER","","","4.35","4.35","4.35 (6)"]
["","Jaarlijks energieverbruik","","kWu/a","965.517","965.517"]
["","Vermogen","Pdesign","kW","12.00","12.00"]
["","Energieklasse","","","C","C"]
["Verwarming (gematigd klimaat)","Vermogen","Pdesign","kW","7.60","7.60"]
["","SCOP/A","","","3.81","3.81","3.81 (6)"]
["","Energieklasse","","","A","A"]
["","Jaarlijks energieverbruik","","kWu/a","2,791","2,791"]
["Nominaal energierendement","Jaarlijks energieverbruik","","kWu","1,870","1,600","1,870"]
["","EER","","","3.21","3.21","3.21"]
["","COP","","","3.51","3.51","3.51"]
["","Richtlijn Energielabels","Koeling","","A","A","A"]
["","","Verwarming","","B","B","B"]
["Totale verwarmingscapaciteit","Nom.","","kW","13.5","13.5","13.5 (4)"]
["Opmerkingen","","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","(1) - Jaarlijks energieverbruik: op basis van een gemiddelde van 500 bedrijfsuren per jaar bij vollast (nominale omstandigheden)"]
["","","","","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting","(2) - Energielabel: schaalverdeling van A (meest efficiënt) tot G (minst efficiënt)"]
["","","","","","","(3) - Koelen: binnentemp. 27°CDB, 19°CWB; buitentemperatuur. 35°CDB; equivalente leidinglengte: 5 m; hoogteverschil: 0m"]
["","","","","","","(4) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5 m; hoogteverschil: 0m"]
["","","","","","","(5) - Jaarlijks energieverbruik is conform richtlijn 2002/31/EC inzake energielabels"]
["","","","","","","(6) - SEER en SCOP zijn conform EN 14825"]
["","","","","","","(7) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting"]