{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":9,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3"]
[]
[]
[]
[]
["","","","","","FDXM25F3V1B","FDXM35F3V1B","FDXM50F3V1B","FDXM60F3V1B"]
["Opgenomen vermogen","Koelen","","Nom.","kW","0.036","0.036","0.060","0.060"]
["","Verwarmen","","Nom.","kW","0.036","0.036","0.060","0.060"]
["Afmetingen","Unit","","Hoogte","mm","200","200","200","200"]
["","","","Breedte","mm","750","750","1150","1150"]
["","","","Diepte","mm","620","620","620","620"]
["Gewicht","Unit","","","kg","21","21","28","28"]
["Ventilator-","Luchthoeveelheid","Koelen","Hoog","m³/min","8.7","8.7","15.8","16.0"]
["Ventilator","Luchtdebiet","Koeling","Middelhoog","m³/min","8.0","8.0","14.6","14.8"]
["Ventilator-","Luchthoeveelheid","Koelen","Laag","m³/min","7.3","7.3","13.3","13.5"]
["","","Verwarmen","Hoog","m³/min","8.7","8.7","15.8","16.0"]
["Ventilator","Luchtdebiet","Verwarming","Middelhoog","m³/min","8.0","8.0","14.6","14.8"]
["Ventilator-","Luchthoeveelheid","Verwarmen","Laag","m³/min","7.3","7.3","13.3","13.5"]
["Ventilator","Externe statische druk","","Nom.","Pa","30","30","40","40"]
["Geluidsvermogenniveau","Koelen","","","dB(A)","53","53","55","56"]
["","Verwarmen","","","dB(A)","53","53","55","56"]
["Geluidsdrukniveau op 1 m","Koelen","","Hoog","dB(A)","35","35","38","38"]
["Geluidsdrukniveau","Koeling","","Middelhoog","dB(A)","33","33","35","35"]
["Geluidsdrukniveau op 1 m","Koelen","","Laag","dB(A)","27","27","30","30"]
["","Verwarmen","","Hoog","dB(A)","35","35","38","38"]
["Geluidsdrukniveau","Verwarming","","Middelhoog","dB(A)","33","33","35","35"]
["Geluidsdrukniveau op 1 m","Verwarmen","","Laag","dB(A)","27","27","30","30"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","6.35","6.35","6.35","6.35"]
["","Gas","","Buitendiameter","mm","9.50","9.50","12.70","12.70"]
["","Drainage","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Standaard-accessoires","Installation manual","","","","1","1","1","1"]
["","Washer for hanger bracket","","","","8","8","8","8"]
["","Operation manual","","","","1","1","1","1"]
["","Clamp metal","","","","1","1","1","1"]
["","Clamps","","","","6","6","6","6"]
["","Drain hose","","","","1","1","1","1"]
["","Luchtfilter","","","","1","1","1","1"]
["","Insulation for fitting","","","","1","1","1","1"]
["","Screws for duct flanges","","","","1","1","1","1"]
["","Sealing material","","","","2","2","2","2"]
["","Sealing pad","","","","1","1","1","1"]
["","Washer fixing plate","","","","4","4","4","4"]
["Voeding","Fase","","","","1~","1~","1~","1~"]
["Spanningsvorm","Frequentie","","","Hz","50","50","50","50"]
["","Spanning","","","V","220-240","220-240","220-240","220-240"]