{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":9,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9"]
[]
[]
[]
[]
["","","","","","FDXM25F3V1B9","FDXM35F3V1B9","FDXM50F3V1B9","FDXM60F3V1B9"]
["Geluidsdrukniveau op 1 m","Verwarmen","","Hoog","dB(A)","35.0","35.0","","38.0"]
["","","","Middelhoog","dB(A)","33.0","33.0","","35.0"]
["","","","Laag","dB(A)","27.0","27.0","","30.0"]
["","Koelen","","Middelhoog","dB(A)","33.0","33.0","","35.0"]
["","","","Laag","dB(A)","27.0","27.0","","30.0"]
["","","","Hoog","dB(A)","35.0","35.0","","38.0"]
["Standaard-accessoires","Montagehandleiding","","","","1","1","","1"]
["","Bedieningshandleiding","","","","1","1","","1"]
["","Isolatie voor fitting","","","","1","1","","1"]
["","Afdichtingskussen","","","","1","1","","1"]
["","Klemmetaal","","","","1","1","","1"]
["","Afvoerslang","","","","1","1","","1"]
["","Sluitring voor ophangbeugel","","","","8","8","","8"]
["","Afdichtingsmateriaal","","","","2","2","","2"]
["","Klemmen","","","","6","6","","6"]
["","Sluitring bevestigingsplaat","","","","4","4","","4"]
["","Schroeven voor kanaalflenzen","","","","1","1","","1"]
["","Luchtfilter","","","","1","1","","1"]
["Piping connections","Vloeistof","","Buitendiameter","mm","6.35","6.35","","6.35"]
["","Gas","","Buitendiameter","mm","9.50","9.50","","12.70"]
["","Drainage","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","","VP20 (I.D. 20/O.D. 26)"]
["Opgenomen vermogen","Koelen","","Nom.","kW","0.036","0.036","","0.060"]
["","Verwarmen","","Nom.","kW","0.036","0.036","","0.060"]
["Geluidsvermogenniveau","Koelen","","","dB(A)","53.0","53.0","","56.0"]
["","Verwarmen","","","dB(A)","53.0","53.0","","56.0"]
["Afmetingen","Unit","","Breedte","mm","750","750","","1,150"]
["","","","Diepte","mm","620","620","","620"]
["","","","Hoogte","mm","200","200","","200"]
["Gewicht","Unit","","","kg","21","21","","28"]
["Ventilator","Externe statische druk","","Nom.","Pa","30","30","","40"]
["","Luchthoeveelheid","Verwarmen","Hoog","m³/min","8.7","8.7","","16.0"]
["","","","Middelhoog","m³/min","8.0","8.0","","14.8"]
["","","","Laag","m³/min","7.3","7.3","","13.5"]
["","","Koelen","Laag","m³/min","7.3","7.3","","13.5"]
["","","","Middelhoog","m³/min","8.0","8.0","","14.8"]
["","","","Hoog","m³/min","8.7","8.7","","16.0"]
["Power supply","Fase","","","","1~","1~","","1~"]
["","Frequentie","","","Hz","50","50","","50"]
["","Spanning","","","V","220-240","220-240","","220-240"]
["Opmerkingen","","","","","(1) - Voor elektrische gegevens zie afzonderlijke tekening","(1) - Voor elektrische gegevens zie afzonderlijke tekening","","(1) - Voor elektrische gegevens zie afzonderlijke tekening"]
["Opgenomen vermogen","Koelen","","Nom.","kW","","","0.060"]
["","Verwarmen","","Nom.","kW","","","0.060"]
["Afmetingen","Unit","","Hoogte","mm","","","200"]
["","","","Breedte","mm","","","1150"]
["","","","Diepte","mm","","","620"]
["Gewicht","Unit","","","kg","","","28"]
["Ventilator-","Luchthoeveelheid","Koelen","Hoog","m³/min","","","15.8"]
["Ventilator","Luchtdebiet","Koeling","Middelhoog","m³/min","","","14.6"]
["Ventilator-","Luchthoeveelheid","Koelen","Laag","m³/min","","","13.3"]
["","","Verwarmen","Hoog","m³/min","","","15.8"]
["Ventilator","Luchtdebiet","Verwarming","Middelhoog","m³/min","","","14.6"]
["Ventilator-","Luchthoeveelheid","Verwarmen","Laag","m³/min","","","13.3"]
["Ventilator","Externe statische druk","","Nom.","Pa","","","40"]
["Geluidsvermogenniveau","Koelen","","","dB(A)","","","55.0"]
["","Verwarmen","","","dB(A)","","","55.0"]
["Geluidsdrukniveau op 1 m","Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Hoog-=-dB(A)","dB(A)","","","38.0"]
["Geluidsdrukniveau","Koeling","","Middelhoog","dB(A)","","","35.0"]
["Geluidsdrukniveau op 1 m","Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Laag-=-dB(A)","dB(A)","","","30.0"]
["","Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Hoog-=-dB(A)","dB(A)","","","38.0"]
["Geluidsdrukniveau","Verwarming","","Middelhoog","dB(A)","","","35.0"]
["Geluidsdrukniveau op 1 m","Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Laag-=-dB(A)","dB(A)","","","30.0"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","","","6.35"]
["","Gas","","Buitendiameter","mm","","","12.70"]
["","Drainage","","","","","","VP20 (I.D. 20/O.D. 26)"]
["Standaard-accessoires","Installation manual","","","","","","1"]
["","Washer for hanger bracket","","","","","","8"]
["","Operation manual","","","","","","1"]
["","Clamp metal","","","","","","1"]
["","Clamps","","","","","","6"]
["","Drain hose","","","","","","1"]
["","Luchtfilter","","","","","","1"]
["","Insulation for fitting","","","","","","1"]
["","Screws for duct flanges","","","","","","1"]
["","Sealing material","","","","","","2"]
["","Sealing pad","","","","","","1"]
["","Washer fixing plate","","","","","","4"]
["Voeding","Fase","","","","","","1~"]
["Spanningsvorm","Frequentie","","","Hz","","","50"]
["","Spanning","","","V","","","220-240"]