{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":8,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F9 / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FDXS50F2VEB9 / FDXS50F2VEB9 / RZQG71L8Y1B","FDXS50F2VEB9 / FDXS50F2VEB9 / FDXS50F2VEB9 / RZQG100L8Y1B","FDXS50F2VEB9 / FDXS50F2VEB9 / RZQG100L8Y1B","FDXS50F2VEB9 / FDXS50F2VEB9 / FDXS50F2VEB9 / RZQG125L8Y1B (Archived)"]
["Koeling","SEER","","","4.80","5.10"]
["","Jaarlijks energieverbruik","","kWu/a","496","652"]
["","Vermogen","Pdesign","kW","6.80","9.50"]
["","Energieklasse","","","B","B"]
["Verwarming (gematigd klimaat)","Vermogen","Pdesign","kW","6.00","11.30"]
["","SCOP/A","","","3.80","3.80"]
["","Energieklasse","","","A","A"]
["","Jaarlijks energieverbruik","","kWu/a","2,211","4,164"]
["Koeling","Koeling-=-Energieklasse","","","","","B","B"]
["","Vermogen","Pdesign","kW","","","9.5","12.00"]
["","SEER","","","","","5.1","5.10"]
["","Jaarlijks energieverbruik","","kWu/a","","","652","824"]
["Verwarming (gematigd klimaat)","Energieklasse","","","","","A","A"]
["","Vermogen","Pdesign","kW","","","11.3","12.71"]
["","SCOP/A","","","","","3.8","3.80"]
["","Jaarlijks energieverbruik","","kWu/a","","","4164","4683"]
["Bereik van het energierendement","","","","","","A+++ ~ D","A+++ ~ D"]
["Opmerkingen","","","","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU"]
["Outdoor unit","","","","","","","RZQG125L8Y1"]