{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A9 / RXM-A"]
[]
[]
[]
[]
["","","","","FFA50A2VEB9 / RXM50A5V1B","FFA60A2VEB9 / RXM60A5V1B"]
["Totale koelcapaciteit","Nom.","","kW","5.00","5.7"]
["Totale verwarmingscapaciteit","Nom.","","kW","5.80","7"]
["Nominaal rendement","EER","","","3.24","3.05"]
["","COP","","","3.49","3.41"]
["","Jaarlijks energieverbruik","","kWu","772","931"]
["Nominaal energierendement","Richtlijn Energielabels","Koeling","","A","B"]
["","","Verwarming","","B","B"]
["Koeling","Koeling-=-Energieklasse","","","A+","A+"]
["","Vermogen","Pdesign","kW","5.00","5.7"]
["","SEER","","","5.98","5.76"]
["","Jaarlijks energieverbruik","","kWu/a","293","346"]
["Verwarming (gematigd klimaat)","Energieklasse","","","A","A+"]
["","Vermogen","Pdesign","kW","3.84","3.96"]
["","SCOP/A","","","3.90","4.04"]
["","Pdh-verwarmingsvermogen bij -10 °C","","kW","3.40","3.5"]
["","Jaarlijks energieverbruik","","kWu/a","1378","1373"]
["Opmerkingen","","","","","(1) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemp.: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m."]
["","","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","","(3) - See separate drawing for operation range"]
["","","","","","(4) - See separate drawing for electrical data"]