{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":14,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A9 / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / RZQG100L8Y1B","FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / RZQG125L8Y1B","FFA50A2VEB9 / FFA50A2VEB9 / FFA50A2VEB9 / RZQG125L8Y1B","FFA50A2VEB9 / FFA50A2VEB9 / RZQG100L8Y1B","FFA60A2VEB9 / FFA60A2VEB9 / RZQG125L8Y1B","FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / RZQG100L8Y1B","FFA50A2VEB9 / FFA50A2VEB9 / FFA50A2VEB9 / RZQG100L8Y1B","FFA50A2VEB9 / FFA50A2VEB9 / RZQG71L8Y1B","FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / RZQG71L8Y1B","FFA35A2VEB9 / FFA35A2VEB9 / RZQG71L8Y1B"]
["Bereik van het energierendement","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Totale koelcapaciteit","Nom.","","kW","","","","","","","","6.80","6.80","6.80"]
["Koeling","SEER","","","","","","","","","","5.10","5.10","5.10"]
["","Jaarlijks energieverbruik","","kWu/a","","","","","","","","467","467","467"]
["","Vermogen","Pdesign","kW","","","","","","","","6.80","6.80","6.80"]
["","Energieklasse","","","","","","","","","","A","A","A"]
["Verwarming (gematigd klimaat)","Vermogen","Pdesign","kW","","","","","","","","6.00","6.00","6.00"]
["","SCOP/A","","","","","","","","","","3.80","3.80","3.80"]
["","Energieklasse","","","","","","","","","","A","A","A"]
["","Jaarlijks energieverbruik","","kWu/a","","","","","","","","2,211","2,211","2,211"]
["Nominaal energierendement","EER","","","","","","","","","","3.38","3.38","3.38"]
["Opmerkingen","","","","","","","","","","","(1) - Zie afzonderlijke afbeelding voor bedrijfsbereik","(1) - Zie afzonderlijke afbeelding voor bedrijfsbereik","(1) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemperatuur: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m."]
["","","","","","","","","","","","(2) - Voor elektrische gegevens zie afzonderlijke tekening","(2) - Voor elektrische gegevens zie afzonderlijke tekening","(2) - Nominale verwarmingscapaciteiten gebaseerd op: binnentemperatuur: 20°CDB, buitentemperatuur: 7°CDB/6°CWB, equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0m."]
["","","","","","","","","","","","","","(3) - Zie afzonderlijke afbeelding voor bedrijfsbereik"]
["","","","","","","","","","","","","","(4) - Voor elektrische gegevens zie afzonderlijke tekening"]