{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":7,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A(9) / RQ-BV3"]
[]
[]
[]
[]
["","","","","FHA71AVEB99 / RQ71B8V3B","FHA71AVEB99 / RQ71B2V3B","FHA100AVEB9 / RQ100B8V3B"]
["Koelvermogen","Nom.","","kW","7.1 (2)","7.1 (2)","9.8 (2)"]
["Leidingaansluitingen","Vloeistof","Buitendiameter","mm","9.52","10","10"]
["","Gas","Buitendiameter","mm","15.90","15.90","15.90"]
["","Drainage","","mm","26","26","26"]
["Nominaal energierendement","EER","","","2.63","2.63","2.61"]
["","Jaarlijks energieverbruik","","kWu","1,350","1,350","1,875"]
["","COP","","","2.81","2.81","2.71"]
["","Richtlijn Energielabels","Koeling","","D","D","D"]
["","","Verwarming","","D","D","E"]
["Verwarmingscapaciteit","Nom.","","kW","8.0 (5)","8.0 (5)","11.2 (5)"]
["Opmerkingen","","","","(1) - Koelen: binnentemp. 27°CDB, 19°CWB; buitentemperatuur. 35°CDB; equivalente leidinglengte: 5 m; hoogteverschil: 0m","(1) - Koelen: binnentemp. 27°CDB, 19°CWB; buitentemperatuur. 35°CDB; equivalente leidinglengte: 5 m; hoogteverschil: 0m","(1) - Koelen: binnentemp. 27°CDB, 19°CWB; buitentemperatuur. 35°CDB; equivalente leidinglengte: 5 m; hoogteverschil: 0m"]
["","","","","(2) - Koelen: binnentemp. 27°CDB, 19°CWB; buitentemperatuur. 35°CDB; equivalente leidinglengte: 7,5m (horizontaal); hoogteverschil: 0m","(2) - Koelen: binnentemp. 27°CDB, 19°CWB; buitentemperatuur. 35°CDB; equivalente leidinglengte: 7,5m (horizontaal); hoogteverschil: 0m","(2) - Koelen: binnentemp. 27°CDB, 19°CWB; buitentemperatuur. 35°CDB; equivalente leidinglengte: 7,5m (horizontaal); hoogteverschil: 0m"]
["","","","","(3) - Koelen: binnentemp. 27°CDB, 19°CWB; buitentemperatuur. 35°CDB; equivalente leidinglengte: 7,5m; hoogteverschil: 0m","(3) - Koelen: binnentemp. 27°CDB, 19°CWB; buitentemperatuur. 35°CDB; equivalente leidinglengte: 7,5m; hoogteverschil: 0m","(3) - Koelen: binnentemp. 27°CDB, 19°CWB; buitentemperatuur. 35°CDB; equivalente leidinglengte: 7,5m; hoogteverschil: 0m"]
["","","","","(4) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5 m; hoogteverschil: 0m","(4) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5 m; hoogteverschil: 0m","(4) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5 m; hoogteverschil: 0m"]
["","","","","(5) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 7,5m; hoogteverschil: 0m","(5) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 7,5m; hoogteverschil: 0m","(5) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 7,5m; hoogteverschil: 0m"]