{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":6,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RZASG-MY1"]
[]
[]
[]
[]
["","","","","FHA35AVEB / FHA35AVEB / FHA35AVEB / RZASG100M7Y1B","FHA50AVEB / FHA50AVEB / RZASG100M7Y1B"]
["Buitendeel","","","","RZASG100M7Y1B","RZASG100M7Y1B"]
["Totale koelcapaciteit","Nom.","","kW","9.50","9.50"]
["Totale verwarmingscapaciteit","Nom.","","kW","10.8","10.8"]
["Koeling","Koeling-=-Energieklasse","","","A++","A+"]
["","Vermogen","Pdesign","kW","9.50","9.50"]
["","SEER","","","7.26","5.79"]
["","Jaarlijks energieverbruik","","kWu/a","458","574"]
["Verwarming (gematigd klimaat)","Energieklasse","","","A+","A"]
["","Vermogen","Pdesign","kW","6.00","6.00"]
["","SCOP/A","","","4.02","3.92"]
["","Jaarlijks energieverbruik","","kWu/a","2090","2143"]
["Opmerkingen","","","","(1) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemp.: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m.","(1) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemp.: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]