{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":8,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTX-J3"]
[]
[]
[]
[]
["","","","","","FTX20J3V1B","FTX25J3V1B","FTX35J3V1B"]
["Opgenomen vermogen","Koelen","","Nom.","kW","0.03","0.030","0.030"]
["","Verwarmen","","Nom.","kW","0.04","0.040","0.040"]
["Behuizing","Kleur","","","","Wit","Wit","Wit"]
["Afmetingen","Unit","","Hoogte","mm","198","198","198"]
["","","","Breedte","mm","770","770","770"]
["","","","Diepte","mm","283","283","283"]
["Gewicht","Unit","","","kg","7","7.00","7.00"]
["Ventilator-","Luchthoeveelheid","Koelen","Hoog","m³/min","9.1","9.2","9.3"]
["Ventilator","Luchtdebiet","Koeling","Middelhoog","m³/min","7.4","7.6","7.7"]
["Ventilator-","Luchthoeveelheid","Koelen","Laag","m³/min","5.9","6.0","6.1"]
["","","","Fluisterstille werking","m³/min","4.7","4.8","4.9"]
["","","Verwarmen","Hoog","m³/min","9.4","9.7","10.1"]
["Ventilator","Luchtdebiet","Verwarming","Middelhoog","m³/min","7.8","8.0","8.4"]
["Ventilator-","Luchthoeveelheid","Verwarmen","Laag","m³/min","6.3","6.3","6.7"]
["","","","Fluisterstille werking","m³/min","5.5","5.5","5.7"]
["Geluidsvermogenniveau","Koelen","","","dB(A)","55","55","58"]
["","Verwarmen","","","dB(A)","55","55","58"]
["Geluidsdrukniveau op 1 m","Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Hoog-=-dB(A)","dB(A)","39","40","41"]
["Geluidsdrukniveau","Koeling","","Middelhoog","dB(A)","33","33","34"]
["Geluidsdrukniveau op 1 m","Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Laag-=-dB(A)","dB(A)","25","26","27"]
["","","","Geluidsdrukniveau op 1 m-=-Koelen-=-Fluisterstille werking-=-dB(A)","dB(A)","22","22","23"]
["","Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Hoog-=-dB(A)","dB(A)","39","40","41"]
["Geluidsdrukniveau","Verwarming","","Middelhoog","dB(A)","34","34","35"]
["Geluidsdrukniveau op 1 m","Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Laag-=-dB(A)","dB(A)","28","28","29"]
["","","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Fluisterstille werking-=-dB(A)","dB(A)","25","25","26"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","6.35","6.35","6.35"]
["","Gas","","Buitendiameter","mm","9.5","9.50","9.50"]
["","Drainage","","","","18","18","18"]
["Besturingssystemen","Infrared remote control","","","","ARC433A87","ARC433A87","ARC433A87"]
["Standaard-accessoires","Installation manual","","","","1","1","1"]
["","Wireless remote control","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2"]
["","Indoor unit fixing screws","","","","2","2","2"]
["","Mounting plate","","","","1","1","1"]
["","Remote control holder","","","","1","1","1"]
["Voeding","Naam","","","","V1","V1","V1"]
["","Fase","","","","1~","1~","1~"]
["Spanningsvorm","Frequentie","","","Hz","50","50","50"]
["","Spanning","","","V","220-240","220-240","220-240"]