{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":10,"n_cols":7,"rows_kept":10,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXC-A / RXC-A"]
[]
[]
[]
[]
["","","","FTXC25AV1B / RXC25AV1B","FTXC35AV1B / RXC35AV1B","FTXC50AV1B / RXC50AV1B","FTXC60AV1B / RXC60AV1B"]
["Koelcapaciteit","Nom.","kW","2.56","3.37","5.48","6.23"]
["Nominaal energierendement","EER","","3.08","2.63","3.54","3.44"]
["","COP","","3.64","3.58","3.70","3.93"]
["Totale verwarmingscapaciteit","Nom.","kW","2.84","3.58","5.62","6.40"]