{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":8,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXC-A"]
[]
[]
[]
[]
["","","","","FTXC25AV1B","FTXC35AV1B","FTXC50AV1B","FTXC60AV1B"]
["Geluidsdrukniveau op 1 m","Koelen","Fluisterstille werking","dB(A)","21","22","32","33"]
["","","Superhoog","dB(A)","41","42","44","46"]
["","","Laag","dB(A)","29","30","35","37"]
["","","Hoog","dB(A)","40","41","40","43"]
["Standaard-accessoires","Montagehandleiding","","","Montagehandleiding","Montagehandleiding","Montagehandleiding","Montagehandleiding"]
["","Bedieningshandleiding","","","Bedieningshandleiding","Bedieningshandleiding","Bedieningshandleiding","Bedieningshandleiding"]
["","Draadloze afstandsbediening","","","Draadloze afstandsbediening","Draadloze afstandsbediening","Draadloze afstandsbediening","Draadloze afstandsbediening"]
["","Batterijen","","","Batterijen","Batterijen","Batterijen","Batterijen"]
["","Afstandsbedieningshouder","","","Afstandsbedieningshouder","Afstandsbedieningshouder","Afstandsbedieningshouder","Afstandsbedieningshouder"]
["","Montageplaat","","","Montageplaat","Montageplaat","Montageplaat","Montageplaat"]
["","Filters van titaan-apatiet","","","Filters van titaan-apatiet","Filters van titaan-apatiet","Filters van titaan-apatiet","Filters van titaan-apatiet"]
["Piping connections","Vloeistof","Buitendiameter","mm","6.35","6.35","6.35","6.35"]
["","Gas","Buitendiameter","mm","9.5","9.5","12.7","12.7"]
["","Afvoer","","","OD16,5","OD16,5","OD16,5","OD16,5"]
["Opgenomen vermogen","Koelen","Nom.","kW","693","1,060","1,668","1,931"]
["","Verwarmen","Nom.","kW","700","950","1,550","1,680"]
["Geluidsvermogenniveau","Koelen","","dB(A)","53","54","55","61"]
["Afmetingen","Unit","Breedte","mm","859","859","1,124","1,124"]
["","","Diepte","mm","209","209","237","237"]
["","","Hoogte","mm","288","288","310","310"]
["Omkasting","Materiaal","","","Schokpolystyreen","Schokpolystyreen","Schokpolystyreen","Schokpolystyreen"]
["","Kleur","","","Wit","Wit","Wit","Wit"]
["Gewicht","Unit","","kg","9.0","9.0","14.0","14.0"]
["Ventilator","Externe statische druk","Hoog","Pa","0","0","0","0"]
["","","Nom.","Pa","0","0","0","0"]
["","","Laag","Pa","0","0","0","0"]
["","","Superhoog","Pa","0","0","0","0"]
["Power supply","Fase","","","1~","1~","1~","1~"]
["","Frequentie","","Hz","50","50","50","50"]
["","Naam","","","V1","V1","V1","V1"]
["","Spanning","","V","220-240","220-240","220-240","220-240"]