{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-B"]
[]
[]
[]
[]
["","","","","FTXF20B5V1B","FTXF25B5V1B"]
["Geluidsdrukniveau op 1 m","Verwarmen","Hoog","dB(A)","39","40"]
["","","Middelhoog","dB(A)","34","34"]
["","","Fluisterstille werking","dB(A)","21","21"]
["","","Laag","dB(A)","28","28"]
["","Koelen","Middelhoog","dB(A)","33","33"]
["","","Fluisterstille werking","dB(A)","20","20"]
["","","Laag","dB(A)","25","26"]
["","","Hoog","dB(A)","39","40"]
["Standaard-accessoires","Montagehandleiding","","","1","1"]
["","Bedieningshandleiding","","","1","1"]
["","Infrarood-afstandsbediening","","","1","1"]
["","AAA drogecelbatterij","","","2","2"]
["","Afstandsbedieningshouder","","","1","1"]
["","Montageplaat","","","1","1"]
["","Montageschroeven binnenunit","","","2","2"]
["Regelsystemen","Bedrade afstandsbediening","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["","Infrared remote control","","","ARC470A1","ARC470A1"]
["Koelleidingmaten","Vloeistof","Buitendiameter","mm","6.35","6.35"]
["","Gas","Buitendiameter","mm","9.50","9.50"]
["","Afvoer","","","18","18"]
["Opgenomen vermogen","Koelen","Nom.","kW","0.017","0.019"]
["","Verwarmen","Nom.","kW","0.020","0.020"]
["Geluidsvermogenniveau","Koelen","","dB(A)","55","55"]
["","Verwarmen","","dB(A)","55","55"]
["Afmetingen","Unit","Breedte","mm","770","770"]
["","","Diepte","mm","225","225"]
["","","Hoogte","mm","286","286"]
["Behuizing","Kleur","","","Wit","Wit"]
["Gewicht","Unit","","kg","8.50","8.50"]
["Power supply","Fase","","","1~","1~"]
["","Frequentie","","Hz","50","50"]
["","Spanning","","V","220-240","220-240"]