{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":9,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-E"]
[]
[]
[]
[]
["","","","","","FTXF20E5V1B","FTXF25E5V1B","FTXF35E5V1B","FTXF42E5V1B"]
["Opgenomen vermogen","Koelen","","Nom.","kW","0.023","0.023","0.029","0.040"]
["","Verwarmen","","Nom.","kW","0.023","0.023","0.029","0.040"]
["Behuizing","Kleur","","","","Wit","Wit","Wit","Wit"]
["Afmetingen","Unit","","Hoogte","mm","286","286","286","286"]
["","","","Breedte","mm","770","770","770","770"]
["","","","Diepte","mm","225","225","225","225"]
["Gewicht","Unit","","","kg","8","8","8.5","9.00"]
["Ventilator-","Luchthoeveelheid","Koelen","Hoog","m³/min","9.8","10","11.5","12.6"]
["Ventilator","Luchtdebiet","Koeling","Middelhoog","m³/min","8","8","8","9"]
["Ventilator-","Luchthoeveelheid","Koelen","Laag","m³/min","6","6.2","6.4","6.9"]
["","","","Fluisterstille werking","m³/min","4.3","4.3","4.4","4.9"]
["","","Verwarmen","Hoog","m³/min","10.4","10.4","11.9","12.8"]
["Ventilator","Luchtdebiet","Verwarming","Middelhoog","m³/min","8.3","8.4","8.6","8.8"]
["Ventilator-","Luchthoeveelheid","Verwarmen","Laag","m³/min","6.2","6.4","6.5","6.7"]
["","","","Fluisterstille werking","m³/min","5.3","5.3","5.3","5.2"]
["Geluidsvermogenniveau","Koelen","","","dB(A)","53","54","54","59.0"]
["","Verwarmen","","","dB(A)","55","55","56","59.0"]
["Geluidsdrukniveau op 1 m","Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Hoog-=-dB(A)","dB(A)","","40","43","45.0"]
["Geluidsdrukniveau","Koeling","","Middelhoog","dB(A)","33","33","34","36.0"]
["Geluidsdrukniveau op 1 m","Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Laag-=-dB(A)","dB(A)","","26","27","30.0"]
["","","","Geluidsdrukniveau op 1 m-=-Koelen-=-Fluisterstille werking-=-dB(A)","dB(A)","","20","20","22.0"]
["","Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Hoog-=-dB(A)","dB(A)","","40","40","44.0"]
["Geluidsdrukniveau","Verwarming","","Middelhoog","dB(A)","34","34","35","34.0"]
["Geluidsdrukniveau op 1 m","Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Laag-=-dB(A)","dB(A)","","28","29","28.0"]
["","","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Fluisterstille werking-=-dB(A)","dB(A)","","21","21","22.0"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","6","6","6","6"]
["","Gas","","Buitendiameter","mm","9.5","9.5","9.5","9.50"]
["","Drainage","","","","18","18","18","18"]
["Regelsystemen","IR-afstandsbediening","","","","ARC470A1","ARC470A1","ARC470A1","ARC470A1"]
["","Bedrade afstandsbediening","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Standaard-accessoires","Installation manual","","","","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2"]
["","General safety precautions","","","","1","1","1","1"]
["","Operation manual","","","","1","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1"]
["Voeding","Fase","","","","1~","1~","1~","1~"]
["Spanningsvorm","Frequentie","","","Hz","50","50","50","50"]
["","Spanning","","","V","220-440","220-440","220-440","220-440"]
["Geluidsdrukniveau op 1 m","Koelen","","Hoog","dB(A)","39"]
["","","","Laag","dB(A)","25"]
["","","","Fluisterstille werking","dB(A)","20"]
["","Verwarmen","","Hoog","dB(A)","39"]
["","","","Laag","dB(A)","28"]
["","","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Fluisterstille werking-=-dBA","dB(A)","21"]