{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":57,"n_cols":12,"rows_kept":57,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-F"]
[]
[]
[]
[]
["","","","","","FTXF42F5V1B","FTXF71F2V1B","FTXF20F5V1B (Archived)","FTXF25F5V1B (Archived)","FTXF35F5V1B (Archived)","FTXF50F5V1B (Archived)","FTXF60F2V1B (Archived)"]
["Opgenomen vermogen","Koelen","","Nom.","kW","0.04","0.032","0.023","0.023","0.029","0.04","0.032"]
["","Verwarmen","","Nom.","kW","0.04","0.035","0.023","0.023","0.029","0.04","0.035"]
["Behuizing","Kleur","","","","Wit","Wit","Wit","Wit","Wit","Wit","Wit"]
["Afmetingen","Unit","","Hoogte","mm","286","295","286","286","286","286","295"]
["","","","Breedte","mm","770","990","770","770","770","770","990"]
["","","","Diepte","mm","225","263","225","225","225","225","263"]
["Gewicht","Unit","","","kg","9","13.5","8","8","8.5","9","13.5"]
["Ventilator-","Luchthoeveelheid","Koelen","Hoog","m³/min","12.6","17.3","9.8","10","11.5","12.6","17.3"]
["Ventilator","Luchtdebiet","Koeling","Middelhoog","m³/min","9","14.8","8","8","8","9","14.8"]
["Ventilator-","Luchthoeveelheid","Koelen","Laag","m³/min","6.9","12.2","6","6.2","6.4","7.2","12.2"]
["","","","Fluisterstille werking","m³/min","4.9","10.7","4.3","4.3","4.4","6.4","10.7"]
["","","Verwarmen","Hoog","m³/min","12.8","17.9","10.4","10.4","11.9","12.8","17.9"]
["Ventilator","Luchtdebiet","Verwarming","Middelhoog","m³/min","8.8","15.8","8.3","8.4","8.6","9.6","15.8"]
["Ventilator-","Luchthoeveelheid","Verwarmen","Laag","m³/min","6.7","12.8","6.2","6.4","6.5","7.2","12.8"]
["","","","Fluisterstille werking","m³/min","5.2","11.3","5.3","5.3","5.3","6.4","11.3"]
["Geluidsvermogenniveau","Koelen","","","dB(A)","59","62","53","54","54","59","60"]
["","Verwarmen","","","dB(A)","59","62","55","55","56","59","62"]
["Geluidsdrukniveau op 1 m","Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Hoog-=-dB(A)","dB(A)","45","46"]
["Geluidsdrukniveau","Koeling","","Middelhoog","dB(A)","36","42","33","33","34","39","41"]
["Geluidsdrukniveau op 1 m","Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Laag-=-dB(A)","dB(A)","30","37"]
["","","","Geluidsdrukniveau op 1 m-=-Koelen-=-Fluisterstille werking-=-dB(A)","dB(A)","22","34"]
["","Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Hoog-=-dB(A)","dB(A)","44","45"]
["Geluidsdrukniveau","Verwarming","","Middelhoog","dB(A)","34","41","34","34","35","38","40"]
["Geluidsdrukniveau op 1 m","Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Laag-=-dB(A)","dB(A)","28","36"]
["","","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Fluisterstille werking-=-dB(A)","dB(A)","22","33"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","6","6.35","6","6","6","6","6.35"]
["","Gas","","Buitendiameter","mm","9.5","12.7","9.5","9.5","9.5","12.7","12.7"]
["","Drainage","","","","18","18","18","18","18","18","18"]
["Regelsystemen","IR-afstandsbediening","","","","ARC480A93","ARC470A1","ARC480A93","ARC480A93","ARC480A93","ARC480A93","ARC470A1"]
["","Bedrade afstandsbediening","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Standaard-accessoires","Installation manual","","","","1","1","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2","2","2","2"]
["","General safety precautions","","","","1","","1","1","1","1"]
["","Operation manual","","","","1","1","1","1","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1","1","1"]
["Voeding","Naam","","","","","V1","","","","","V1"]
["","Fase","","","","1~","1~","1~","1~","1~","1~","1~"]
["Spanningsvorm","Frequentie","","","Hz","50","50","50","50","50","50","50"]
["","Spanning","","","V","220-440","220-240","220-440","220-440","220-440","220-440","220-240"]
["Opmerkingen","","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","","(1) - Koelen: binnentemp. 27°CDB, 19°CWB; buitentemperatuur. 35°CDB; equivalente leidinglengte: 5 m; hoogteverschil: 0m","(1) - Koelen: binnentemp. 27°CDB, 19°CWB; buitentemperatuur. 35°CDB; equivalente leidinglengte: 5 m; hoogteverschil: 0m","(1) - Koelen: binnentemp. 27°CDB, 19°CWB; buitentemperatuur. 35°CDB; equivalente leidinglengte: 5 m; hoogteverschil: 0m","(1) - Koelen: binnentemp. 27°CDB, 19°CWB; buitentemperatuur. 35°CDB; equivalente leidinglengte: 5 m; hoogteverschil: 0m"]
["","","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m (horizontal)","","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5 m (horizontaal)","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5 m (horizontaal)","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5 m (horizontaal)","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5 m (horizontaal)"]
["","","","","","(3) - See separate drawing for electrical data","","(3) - Voor elektrische gegevens zie afzonderlijke tekening","(3) - Voor elektrische gegevens zie afzonderlijke tekening","(3) - Voor elektrische gegevens zie afzonderlijke tekening","(3) - Voor elektrische gegevens zie afzonderlijke tekening"]
["Geluidsdrukniveau op 1 m","Koelen","","Hoog","dB(A)","","","39","40","43","45","45"]
["","","","Laag","dB(A)","","","25","26","27","34","36"]
["","","","Fluisterstille werking","dB(A)","","","20","20","20","31","33"]
["","Verwarmen","","Hoog","dB(A)","","","39","40","40","44","44"]
["","","","Laag","dB(A)","","","28","28","29","33","35"]
["","","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Fluisterstille werking-=-dBA","dB(A)","","","21","21","21","30","32"]