{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-M9 / 2MXM-A9"]
[]
[]
[]
[]
["","","","","FTXP20M5V1B9 / FTXP20M5V1B9 / 2MXM40A2V1B9","FTXP20M5V1B9 / FTXP20M5V1B9 / 2MXM50A2V1B9"]
["Totale koelcapaciteit","Nom.","","kW","4"]
["Totale verwarmingscapaciteit","Nom.","","kW","4.2"]
["Nominaal rendement","EER","","","3.71"]
["","COP","","","3.75"]
["","Jaarlijks energieverbruik","","kWh","539"]
["Nominaal energierendement","Richtlijn Energielabels","Koeling","","A"]
["","","Verwarming","","A"]
["Koeling","Koeling-=-Energieklasse","","","A++"]
["","Vermogen","Pdesign","kW","4"]
["","SEER","","","7.74"]
["","Jaarlijks energieverbruik","","kWu/a","181"]
["Verwarming (gematigd klimaat)","Energieklasse","","","A+"]
["","Vermogen","Pdesign","kW","3.2"]
["","SCOP/A","","","4.3"]
["","Pdh-verwarmingsvermogen bij -10 °C","","kW","2.46"]
["","Jaarlijks energieverbruik","","kWu/a","1041"]
["Opmerkingen","","","","(1) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemp.: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m.","(1) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemperatuur: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominale verwarmingscapaciteiten gebaseerd op: binnentemperatuur: 20°CDB, buitentemperatuur: 7°CDB/6°CWB, equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - Zie afzonderlijke afbeelding voor bedrijfsbereik"]
["","","","","(4) - See separate drawing for electrical data","(4) - Voor elektrische gegevens zie afzonderlijke tekening"]
["Totale koelcapaciteit","Nom.","","kW","","4.00"]
["Totale verwarmingscapaciteit","Nom.","","kW","","5.20"]
["Nominaal energierendement","Jaarlijks energieverbruik","","kWh","","554"]
["","COP","","","","3.68"]
["","EER","","","","3.61"]
["","Richtlijn Energielabels","Koeling","","","A"]
["","","Verwarming","","","A"]