{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":8,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXZ-N"]
[]
[]
[]
[]
["","","","","","FTXZ25NV1B","FTXZ35NV1B","FTXZ50NV1B"]
["Geluidsdrukniveau op 1 m","Verwarmen","","Hoog","dB(A)","39","42","44"]
["","","","Fluisterstille werking","dB(A)","19","19","24"]
["","","","Laag","dB(A)","28","29","31"]
["","Koelen","","Fluisterstille werking","dB(A)","19","19","23"]
["","","","Laag","dB(A)","26","27","30"]
["","","","Hoog","dB(A)","38","42","47"]
["","","","Nom.","dB(A)","35","36","38"]
["","Koelen","","Nom.","dB(A)","33","35","38"]
["Standaard-accessoires","Luchtzuiverende en reukverdrijvende fotokatalytische filter","","","","1","1","1"]
["","Draadloze afstandsbediening","","","","1","1","1"]
["","Droge batterijen","","","","2","2","2"]
["","Afstandsbedieningshouder","","","","1","1","1"]
["","Montageschroeven binnenunit","","","","3","3","3"]
["","Montageplaat","","","","1","1","1"]
["Regelsystemen","Infrared remote control","","","","ARC477A1","ARC477A1","ARC477A1"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","6.35","6.35","6.35"]
["","Gas","","Buitendiameter","mm","9.5","9.5","9.5"]
["Opgenomen vermogen","Koelen","","Nom.","kW","0.030","0.030","0.030"]
["","Verwarmen","","Nom.","kW","0.030","0.030","0.030"]
["Sound power level","Koelen","","","dB(A)","54","57","60"]
["","Verwarmen","","","dB(A)","56","57","59"]
["Afmetingen","Unit","","Breedte","mm","798","798","798"]
["","","","Diepte","mm","372","372","372"]
["","","","Hoogte","mm","295","295","295"]
["Behuizing","Kleur","","","","Wit","Wit","Wit"]
["Gewicht","Unit","","","kg","15","15","15"]
["Ventilator","Luchthoeveelheid","Verwarmen","Hoog","m³/min","11.7","13.3","14.4"]
["","","","Laag","m³/min","6.7","6.9","7.7"]
["","","","Fluisterstille werking","m³/min","4.8","4.8","5.9"]
["","","Koelen","Laag","m³/min","5.3","5.6","6.6"]
["","","","Hoog","m³/min","10.7","12.1","15.0"]
["","","","Fluisterstille werking","m³/min","4.0","4.0","4.6"]
["","","","Nom.","m³/min","8.6","9.2","10.7"]
["","","Koelen","Nom.","m³/min","7.5","8.4","9.2"]
["Power supply","Fase","","","","1~","1~","1~"]
["","Naam","","","","V1","V1","V1"]
["","Frequentie","","","Hz","50","50","50"]
["","Spanning","","","V","220-240","220-240","220-240"]
["Opmerkingen","","","","","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","(4) - Voorkant van warmtewisselaar","(4) - Voorkant van warmtewisselaar","(4) - Voorkant van warmtewisselaar"]
["","","","","","(5) - Achterkant van warmtewisselaar","(5) - Achterkant van warmtewisselaar","(5) - Achterkant van warmtewisselaar"]