{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":6,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUQ-C / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FUQ100CVEB / RZQG71L8Y1B","FUQ71CVEB / RZQG71L8Y1B"]
["Koeling","SEER","","","6.50","6.42"]
["","Jaarlijks energieverbruik","","kWu/a","367","371"]
["","Vermogen","Pdesign","kW","6.80","6.80"]
["","Energieklasse","","","A++","A++"]
["Verwarming (gematigd klimaat)","Vermogen","Pdesign","kW","7.60","7.60"]
["","SCOP/A","","","4.20","4.20"]
["","Energieklasse","","","A+","A+"]
["","Jaarlijks energieverbruik","","kWu/a","2,534","2,534"]
["Koelcapaciteit","Nom.","","kW","","6.8"]
["Nominaal energierendement","Jaarlijks energieverbruik","","kWu","","840"]
["","EER","","","","4.05"]
["","COP","","","","4.08"]
["","Richtlijn Energielabels","Koeling","","","A"]
["","","Verwarming","","","A"]
["Totale verwarmingscapaciteit","Nom.","","kW","","7.5"]
["Opmerkingen","","","","","(1) - Jaarlijks energieverbruik is conform richtlijn 2002/31/EC inzake energielabels"]
["","","","","","(2) - SEER en SCOP zijn conform EN 14825"]