{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":7,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUQ-C"]
[]
[]
[]
[]
["","","","","FUQ71CVEB","FUQ100CVEB","FUQ125CVEB"]
["Geluidsdrukniveau op 1 m","Verwarmen","Hoog","dB(A)","41","46","47"]
["","","Nom.","dB(A)","38","42","43"]
["","","Laag","dB(A)","35","39","40"]
["","Koelen","Laag","dB(A)","35","39","40"]
["","","Hoog","dB(A)","41","46","47"]
["","","Nom.","dB(A)","38","42","43"]
["Standaard-accessoires","Montagehandleiding","","","Montagehandleiding","Montagehandleiding","Montagehandleiding"]
["","Bedieningshandleiding","","","Bedieningshandleiding","Bedieningshandleiding","Bedieningshandleiding"]
["","Verklaring van conformiteit","","","Verklaring van conformiteit","Verklaring van conformiteit","Verklaring van conformiteit"]
["","Afvoerslang","","","Afvoerslang","Afvoerslang","Afvoerslang"]
["","Klemmetaal","","","Klemmetaal","Klemmetaal","Klemmetaal"]
["","Sluitring voor ophangbeugel","","","Sluitring voor ophangbeugel","Sluitring voor ophangbeugel","Sluitring voor ophangbeugel"]
["","Klemmen","","","Klemmen","Klemmen","Klemmen"]
["","Sluitklem","","","Sluitklem","Sluitklem","Sluitklem"]
["","Isolatie en dichtingsmateriaal voor koppelverbindingen","","","Isolatie en dichtingsmateriaal voor koppelverbindingen","Isolatie en dichtingsmateriaal voor koppelverbindingen","Isolatie en dichtingsmateriaal voor koppelverbindingen"]
["","Bochtstuk","","","Bochtstuk","Bochtstuk","Bochtstuk"]
["","Montagepatroon","","","Montagepatroon","Montagepatroon","Montagepatroon"]
["","Blokkeermateriaal","","","Blokkeermateriaal","Blokkeermateriaal","Blokkeermateriaal"]
["","L-vormige leiding","","","L-vormige leiding","L-vormige leiding","L-vormige leiding"]
["","Schroeven","","","Schroeven","Schroeven","Schroeven"]
["","Non-woven textiel","","","Non-woven textiel","Non-woven textiel","Non-woven textiel"]
["Regelsystemen","Bedrade afstandsbediening","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["","Infrared remote control","","","BRC7C58","BRC7C58","BRC7C58"]
["Leidingaansluitingen","Vloeistof","Buitendiameter","mm","9.52","9.52","9.52"]
["","Gas","Buitendiameter","mm","15.9","15.9","15.9"]
["","Afvoer","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Sound power level","Koelen","","dB(A)","59","64","65"]
["","Verwarmen","","dB(A)","59","64","65"]
["Afmetingen","Unit","Breedte","mm","950","950","950"]
["","","Diepte","mm","950","950","950"]
["","","Hoogte","mm","198","198","198"]
["Behuizing","Materiaal","","","Hars","Hars","Hars"]
["","Kleur","","","Zuiver wit","Zuiver wit","Zuiver wit"]
["Gewicht","Unit","","kg","25","26","26"]
["Afvoerhoogte","mm","","","600","600","600"]
["Power supply","Fase","","","1~","1~","1~"]
["","Frequentie","","Hz","50/60","50/60","50/60"]
["","Naam","","","VE","VE","VE"]
["","Spanning","","V","220-240/220","220-240/220","220-240/220"]