{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":8,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVA-A / RZASG-MV"]
[]
[]
[]
[]
["","","","","FVA100AMVEB / RZASG100MUV","FVA125AMVEB / RZASG125MUV","FVA71AMVEB / FVA71AMVEB / RZASG140MUV","FVA140AMVEB / RZASG140MUV"]
["Totale koelcapaciteit","Totale koelcapaciteit-=-Nom.-=-kW","","kW","9.5","12.1 (1)","13.4 (1)","13.4 (1)"]
["Totale verwarmingscapaciteit","Totale verwarmingscapaciteit-=-Nom.-=-kW","","kW","10.8 (2)","13.5 (2)","15.5 (2)","15.5 (2)"]
["Koeling","Koeling-=-Energieklasse","","","A+"]
["","Koeling-=-Vermogen","Koeling-=-Vermogen-=-Pdesign-=-kW","kW","9.5","12.1","13.4","13.4"]
["","Koeling-=-SEER","","","5.72","5.52","7.71","5.63"]
["","Koeling-=-Jaarlijks energieverbruik-=-kWu/a","","kWu/a","581","1314","1043","1429"]
["Verwarming (gematigd klimaat)","Verwarming (gematigd klimaat)-=-Energieklasse","","","A"]
["","Verwarming (gematigd klimaat)-=-Vermogen","Verwarming (gematigd klimaat)-=-Vermogen-=-Pdesign-=-kW","kW","6","6","7.8","7.8"]
["","Verwarming (gematigd klimaat)-=-SCOP/A","","","3.83","3.64","4.43","3.81"]
["","Verwarming (gematigd klimaat)-=-Jaarlijks energieverbruik-=-kWu/a","","kWu/a","2193","2308","2467","2866"]
["Opmerkingen","","","","(1) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemp.: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m.","(1) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemp.: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m.","(1) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemp.: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m.","(1) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemp.: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]