{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":9,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVA-A"]
[]
[]
[]
[]
["","","","","","FVA71AMVEB","FVA100AMVEB","FVA125AMVEB","FVA140AMVEB"]
["Totale koelcapaciteit","Totale capaciteit","","Nom.","kW","","","12.10","13.40"]
["Verwarmingscapaciteit","Totaalvermogen","","Nom.","kW","","","13.5","15.5"]
["Behuizing","Kleur","","","","Zuiver wit","Zuiver wit","Zuiver wit","Zuiver wit"]
["Afmetingen","Unit","","Hoogte","mm","1850","1850","1850","1850"]
["","","","Breedte","mm","600","600","600","600"]
["","","","Diepte","mm","270","350","350","350"]
["Gewicht","Unit","","","kg","42","50","50","50"]
["Ventilator-","Luchthoeveelheid","Koelen","Hoog","m³/min","18","28","28","30"]
["Ventilator","Luchtdebiet","Koeling","Middelhoog","m³/min","16","25","26","28"]
["Ventilator-","Luchthoeveelheid","Koelen","Laag","m³/min","14","22","24","26"]
["","","Verwarmen","Hoog","m³/min","18","28","28","30"]
["Ventilator","Luchtdebiet","Verwarming","Middelhoog","m³/min","16","25","26","28"]
["Ventilator-","Luchthoeveelheid","Verwarmen","Laag","m³/min","14","22","24","26"]
["Geluidsvermogenniveau","Koelen","","","dB(A)","55","62","63","65"]
["Geluidsdrukniveau op 1 m","Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Hoog-=-dB(A)","dB(A)","43","50","51","53"]
["Geluidsdrukniveau","Koeling","","Middelhoog","dB(A)","41","47","48","51"]
["Geluidsdrukniveau op 1 m","Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Laag-=-dB(A)","dB(A)","38","44","46","48"]
["","Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Hoog-=-dB(A)","dB(A)","43","50","51","53"]
["Geluidsdrukniveau","Verwarming","","Middelhoog","dB(A)","38","44","46","48"]
["Geluidsdrukniveau op 1 m","Verwarmen","","Nom.","dB(A)","41","47","48","51"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","9.52","9.52","9.52","9.52"]
["","Gas","","Buitendiameter","mm","15.9","15.9","15.9","15.9"]
["","Drainage","","","","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26"]
["Regelsystemen","Bedrade afstandsbediening","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Standaard-accessoires","Installation manual","","","","1","1","1","1"]
["","Hole protection rubber","","","","2","2","2","2"]
["","Cover","","","","1","1","1","1"]
["","Dew proof material","","","","1","1","1","1"]
["","Remote control wiring","","","","1","1","1","1"]
["","Bracket for installation","","","","1","1","1","1"]
["","Operation manual","","","","1","1","1","1"]
["","Bush","","","","1","1","1","1"]
["","Installation pattern","","","","1","1","1","1"]
["","Insulation for fitting for gas pipe","","","","1","1","1","1"]
["","Insulation for fitting for liquid pipe","","","","1","1","1","1"]
["","Screws","","","","5","5","5","5"]
["","Tie-wraps","","","","5","5","5","5"]
["Voeding","Fase","","","","1~","1~","1~","1~"]
["Spanningsvorm","Frequentie","","","Hz","50/60","50/60","50/60","50/60"]
["","Spanning","","","V","220-240/220","220-240/220","220-240/220","220-240/220"]