{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":5,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXM-B / RXM-A"]
[]
[]
[]
[]
["","","","","FVXM50B2V1B / RXM50A5V1B"]
["Totale koelcapaciteit","Min.","","kW","1.4"]
["","Nom.","","kW","5"]
["","Max.","","kW","5.8"]
["Totale verwarmingscapaciteit","Min.","","kW","1.4"]
["","Nom.","","kW","5.8"]
["","Max.","","kW","8.1"]
["Nominaal rendement","EER","","","3.81"]
["","COP","","","3.81"]
["","Jaarlijks energieverbruik","","kWh","656"]
["Nominaal energierendement","Richtlijn Energielabels","Koeling","","A"]
["","","Verwarming","","A"]
["Koeling","Koeling-=-Energieklasse","","","A++"]
["","Vermogen","Pdesign","kW","5"]
["","SEER","","","7.3"]
["","Jaarlijks energieverbruik","","kWu/a","240"]
["Verwarming (gematigd klimaat)","Energieklasse","","","A+"]
["","Vermogen","Pdesign","kW","4.1"]
["","SCOP/A","","","4.31"]
["","Pdh-verwarmingsvermogen bij -10 °C","","kW","3.56"]
["","Jaarlijks energieverbruik","","kWu/a","1330"]
["Opmerkingen","","","","(1) - See separate drawing for operation range"]
["","","","","(2) - See separate drawing for electrical data"]
["","","","","(3) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemp.: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m."]
["","","","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]