{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":59,"n_cols":8,"rows_kept":59,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXM-B"]
[]
[]
[]
[]
["","","","","","FVXM25B2V1B","FVXM50B2V1B","FVXM35B2V1B (Archived)"]
["Opgenomen vermogen","Koelen","","Nom.","kW","0.02","0.03","0.02"]
["","Verwarmen","","Nom.","kW","0.02","0.03","0.03"]
["Behuizing","Kleur","","","","Wit","Wit","Wit"]
["Afmetingen","Unit","","Hoogte","mm","600","600","600"]
["","","","Breedte","mm","750","750","750"]
["","","","Diepte","mm","238","238","238"]
["Gewicht","Unit","","","kg","17","17","17"]
["Ventilator-","Luchthoeveelheid","Koelen","Hoog","m³/min","8.7","11.6","9.2"]
["Ventilator","Luchtdebiet","Koeling","Middelhoog","m³/min","7","9","7"]
["Ventilator-","Luchthoeveelheid","Koelen","Laag","m³/min","4.9","6.6","4.9"]
["","","","Fluisterstille werking","m³/min","4.1","5.4","4.1"]
["","","Verwarmen","Hoog","m³/min","9.2","12.8","9.8"]
["Ventilator","Luchtdebiet","Verwarming","Middelhoog","m³/min","7.2","10","7.2"]
["Ventilator-","Luchthoeveelheid","Verwarmen","Laag","m³/min","5.6","8.4","5.6"]
["","","","Fluisterstille werking","m³/min","4.1","5.9","4.1"]
["Geluidsvermogenniveau","Koelen","","","dB(A)","52","61","53"]
["","Verwarmen","","","dB(A)","52","62","53"]
["Geluidsdrukniveau op 1 m","Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Hoog-=-dB(A)","dB(A)","38","44"]
["Geluidsdrukniveau","Koeling","","Middelhoog","dB(A)","32","38","32"]
["Geluidsdrukniveau op 1 m","Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Laag-=-dB(A)","dB(A)","25","31"]
["","","","Geluidsdrukniveau op 1 m-=-Koelen-=-Fluisterstille werking-=-dB(A)","dB(A)","20","27"]
["","Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Hoog-=-dB(A)","dB(A)","38","46"]
["Geluidsdrukniveau","Verwarming","","Middelhoog","dB(A)","32","40","32"]
["Geluidsdrukniveau op 1 m","Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Laag-=-dB(A)","dB(A)","25","35"]
["","","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Fluisterstille werking-=-dB(A)","dB(A)","19","29"]
["Koelmiddel","GWP","","","","675","675","675"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","6.4","6.4","6.4"]
["","Gas","","Buitendiameter","mm","9.5","12.7","9.5"]
["","Drainage","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Regelsystemen","IR-afstandsbediening","","","","ARC466A90","ARC466A90","ARC466A90"]
["","Bedrade afstandsbediening","","","","BRC073A1","BRC073A1","BRC073A1"]
["Standaard-accessoires","FVXM25B2V1B","","","","1"]
["","Installation manual","","","","1","1","1"]
["","Wireless remote control","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","General safety precautions","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2"]
["","Remote control holder","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Voeding","Naam","","","","V1","V1","V1"]
["","Fase","","","","1~","1~","1~"]
["Spanningsvorm","Frequentie","","","Hz","50","50","50"]
["","Spanning","","","V","220-240","220-240","220-240"]
["Opmerkingen","","","","","(1) - Koelen: binnentemp. 27°CDB, 19°CWB; buitentemperatuur. 35°CDB, 24°CWB; equivalente leidinglengte: 5 m","(1) - Koelen: binnentemp. 27°CDB, 19°CWB; buitentemperatuur. 35°CDB, 24°CWB; equivalente leidinglengte: 5 m","(1) - Koelen: binnentemp. 27°CDB, 19°CWB; buitentemperatuur. 35°CDB, 24°CWB; equivalente leidinglengte: 5 m"]
["","","","","","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5m","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5m","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5m"]
["Standaard-accessoires","FVXM50B2V1B","","","","","1"]
["Geluidsdrukniveau op 1 m","Koelen","","Hoog","dB(A)","","","39"]
["","","","Laag","dB(A)","","","25"]
["","","","Fluisterstille werking","dB(A)","","","20"]
["","Verwarmen","","Hoog","dB(A)","","","39"]
["","","","Laag","dB(A)","","","25"]
["","","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Fluisterstille werking-=-dBA","dB(A)","","","19"]