{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","LRNUN-AY1"]
[]
[]
[]
[]
["","","","","","LRNUN5A7Y1"]
["Standaard-accessoires","Verklaring van conformiteit","","","","1"]
["Gewicht","Unit","","","kg","173"]
["Koudemiddel","GWP","","","","1.0"]
["","Inhoud","","","kg","3.20"]
["Ventilatormotor","Uitgang","","","W","350"]
["Warmtewisselaar","Type","","","","Kruiselings geribd blok"]
["Afmetingen","Unit","","Breedte","mm","635"]
["","","","Diepte","mm","765"]
["","","","Hoogte","mm","1,680"]
["Behuizing","Kleur","","","","Ivoorwit"]
["Ventilator","Type","","","","Schroefventilator"]
["","Luchthoeveelheid","Koelen","Nom.","m³/min","102"]
["","Aantal","","","","1"]
["Power supply","Fase","","","","3N~"]
["","Frequentie","","","Hz","50"]
["","Spanning","","","V","380-415"]
["Opmerkingen","","","","","(1) - LRYEN10A7Y1+LRNUN5A7Y1"]
["","","","","","(2) - Compressor 1"]
["","","","","","(3) - Compressor 2"]
["","","","","","(4) - Compressor 3"]
["","","","","","(5) - Fabrieksvulling van eenheid"]
["","","","","","(6) - Alleen K65 met een drukverschil 120 bar is toegelaten om te gebruiken voor AC-leidingverbindingen."]
["","","","","","(7) - Het overdrukventiel wordt aangegeven als drukmeting."]
["","","","","","(8) - Alleen K65 met een drukverschil 90 bar is toegelaten om te gebruiken voor koelmiddelleidingen."]