{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":6,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","LRYEQ-AY"]
[]
[]
[]
[]
["","","","","","LRYEQ16A7Y1"]
["Standaard-accessoires","Montagehandleiding","","","","1"]
["","Bedieningshandleiding","","","","1"]
["","Aansluitleidingen","","","","1"]
["","Koelmiddellabel voor wetgeving inzake F-gas","","","","1"]
["","Tabel koelmiddelvulling","","","","1"]
["","Meertalige labels gefluoreerde broeikasgassen","","","","1"]
["Gewicht","Unit","","","kg","370"]
["Koudemiddel","Charge","","","TCO2Eq","24.0"]
["","GWP","","","","2,087.5"]
["","Vulling","","","kg","11.5"]
["","Type","","","","R-410A"]
["Ventilatormotor","Output","","","W","750"]
["","Aandrijving","","","","Directe aandrijving"]
["Warmtewisselaar","Type","","","","Kruiselings geribd blok"]
["Afmetingen","Unit","","Breedte","mm","1,240"]
["","","","Diepte","mm","765"]
["","","","Hoogte","mm","1,680"]
["Behuizing","Colour","","","","Ivoorwit"]
["Ventilator","Type","","","","Schroefventilator"]
["","Luchthoeveelheid","Koelen","Nom.","m³/min","230"]
["","Aantal","","","","2"]
["Power supply","Fase","","","","3~"]
["","Frequentie","","","Hz","50"]
["","Spanning","","","V","380-415"]
["Opmerkingen","","","","","(1) - Koelprioriteit-modus: binnentemp. 27°CDB, 19°CNB; buitentemp. 32°CDB; leidinglengte: 7,5 m; hoogteverschil: 0 m"]
["","","","","","(2) - Koelprioriteit-modus: verdampingstemp. -10°C; buitentemp. 32°CDB; Aanzuiging SH: 10°C"]
["","","","","","(3) - Modus 100% warmteterugwinning: binnentemp. 20°CDB; buitentemp. 7°CDB, 6°CNB; koelbelasting 18kW; leidinglengte: 7,5 m; hoogteverschil: 0 m"]
["","","","","","(4) - Verzadigde temperatuur equivalent met aanzuigdruk (koelzijde): -10°C (in gekoelde toestand); aansluitcapaciteit voor binnen-airconditioner: 10 pk, bij warmteterugwinning 100%"]
["","","","","","(5) - Compressor 1"]
["","","","","","(6) - Compressor 2"]
["","","","","","(7) - Compressor 3"]
["","","","","","(8) - Fabrieksvulling van eenheid"]
["","","","","","(9) - Monteer de olieafscheider op 5 m van de buitenunit"]
["","","","","","(10) - Raadpleeg de werkbereik-tekening voor meer informatie"]
["","","","","","(11) - Meer details over standaardaccessoires vindt u in de installatie- en bedieningshandleiding."]
["","","","","","(12) - Bevat gefluoreerde broeikasgassen"]