{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":63,"n_cols":6,"rows_kept":63,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MCK55W"]
[]
[]
[]
[]
["","","","","","MCK55WVM"]
["Type","","","","","Luchtbevochtiger en -reiniger"]
["Toepassing","","","","","Vloermodel"]
["Behuizing","Kleur","","","","Wit"]
["Afmetingen","Unit","","Hoogte","mm","700"]
["","","","Breedte","mm","270"]
["","","","Diepte","mm","270"]
["Gewicht","Unit","","","kg","9.5"]
["Geschikt voor vloeroppervlakte","m²","","","","41 (1), 82 (2)"]
["CADR","m³/u","","","","320"]
["Werking luchtreiniging","Opgenomen vermogen","","Turbo","kW","0.056"]
["","","","M","kW","0.017"]
["","","","L","kW","0.010"]
["","","","Fluisterstil","kW","0.007"]
["Bevochtiging","Opgenomen vermogen","","Turbo","kW","0.058"]
["","","","M","kW","0.019"]
["","","","L","kW","0.014"]
["","","","Fluisterstil","kW","0.011"]
["","Inhoud waterreservoir","","","l","2.7"]
["Geluidsdrukniveau op 1 m","Werking luchtreiniging","","Turbo","dB(A)","53.0"]
["","","","Middelhoog","dB(A)","39.0"]
["","","","Laag","dB(A)","29.0"]
["","","","Fluisterstil","dB(A)","19.0"]
["","Bevochtiging","","Turbo","dB(A)","53.0"]
["","","","Middelhoog","dB(A)","39.0"]
["","","","Laag","dB(A)","33.0"]
["","","","Fluisterstil","dB(A)","25.0"]
["Ventilator-","Luchthoeveelheid","Werking luchtreiniging","Turbo","m³/u","330"]
["","","","Middelhoog","m³/u","192"]
["","","","Laag","m³/u","120"]
["","","","Fluisterstil","m³/u","54"]
["","","Bevochtiging","Turbo","m³/u","330"]
["","","","Middelhoog","m³/u","192"]
["","","","Laag","m³/u","144"]
["","","","Fluisterstil","m³/u","102"]
["Stofvangmethode","","","","","Elektrostatisch HEPA-filter"]
["Ontgeuringsmethode","","","","","Flash streamer + ontgeurende katalysator"]
["Standaard-accessoires","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["","Caster","","","","4"]
["","Humidifying filter","","","","2"]
["","Remote control holder","","","","1"]
["","Remote control lid","","","","1"]
["Voedingskabel","Voedingskabel","","","","1.8"]
["Voeding","Fase","","","","1~"]
["Spanningsvorm","Spanningsvorm-=-Frequentie","","Frequentie","","50/60"]
["","Spanningsvorm-=-Spanning","","Spanning","","220-240/220-230"]
["Bedrijfsstroom","Werking luchtreiniging","Bedrijfsstroom-=-Werking luchtreiniging-=-Turbo","Turbo","","0.50"]
["","","Bedrijfsstroom-=-Werking luchtreiniging-=-Middelhoog","Middelhoog","","0.19"]
["","","Bedrijfsstroom-=-Werking luchtreiniging-=-Laag","Laag","","0.12"]
["","","Bedrijfsstroom-=-Werking luchtreiniging-=-Fluisterstil","Fluisterstil","","0.09"]
["","Bevochtiging","Bedrijfsstroom-=-Bevochtiging-=-Turbo","Turbo","","0.50"]
["","","Bedrijfsstroom-=-Bevochtiging-=-Middelhoog","Middelhoog","","0.20"]
["","","Bedrijfsstroom-=-Bevochtiging-=-Laag","Laag","","0.15"]
["","","Bedrijfsstroom-=-Bevochtiging-=-Fluisterstil","Fluisterstil","","0.13"]
["Opmerkingen","","","","","(1) - De betreffende vloeroppervlakte is voldoende voor het gebruiken van de unit met maximaal toerental van de ventilator (HH). De betreffende vloeroppervlakte verwijst naar de ruimte waarin een bepaald gedeelte stofdeeltjes verwijderd kan worden op 30 minuten. (JEM 1467)"]
["","","","","","(2) - Omgezet naar NRCC-normen van testwaarden overeenkomstig JEM1467."]