{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":6,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","NHY2KOMB-A"]
[]
[]
[]
[]
["","","","","","NHY2KOMB28AA"]
["Sanitair warm water","Opgenomen warmte (thermische netto-waarde) Qnw","Nom","Max","kW","32.3"]
["","","","Min","kW","7.9"]
["","Opgenomen warmte (thermische netto-waarde) Qnw","Nom","Min","kW","7.2"]
["","","","Max","kW","29.1"]
["","Energierendement","","Nom","%","105"]
["Toevoerlucht","Concentrisch","","","","Ja"]
["Sanitair warm water","Algemeen","","Energierendementsklasse waterverwarming","","A"]
["","","","Aangegevens belastingprofiel","","XL"]
["Afmetingen","Unit","Hoogte","Behuizing","mm","650"]
["Behuizing","Materiaal","","","","Voorgelakte metaalplaat"]
["","Kleur","","","","Wit (RAL9010)"]
["Verwarming","Algemeen","","Seizoensrendementsklasse verwarmen","","A"]
["","","","ηs (seizoensrendement van verwarming)","%","93"]
["Centrale verwarming","Opgenomen warmte Qn (thermische bruto-waarde)","Nom","Min","kW","8.0"]
["","","","Max","kW","26.3"]
["","Uitgaand Pn bij 80/60°C","","Min","kW","7.1"]
["","","","Nom","kW","23.1"]
["","Opgenomen warmte Qn (thermische netto-waarde)","Nom","Max","kW","23.7"]
["","","","Min","kW","7.1"]
["","Uitgaand Pn bij 50/30°C","","Min","kW","7.7"]
["","","","Nom","kW","25.4"]
["Gas","Aansluiting","","Diameter","mm","15"]
["","Verbruik (G31)","","Min","m³/u","0.28"]
["","","","Max","m³/u","1.15"]
["","NOx-klasse","","","","6"]
["Opmerkingen","","","","","(1) - 80/60"]
["","","","","","(2) - Ingestelde temp. 60°C"]
["","","","","","(3) - Ingestelde temp. 40℃"]