{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":10,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXF-F"]
[]
[]
[]
[]
["","","","","","RXF20F5V1B (Archived)","RXF25F5V1B (Archived)","RXF35F5V1B (Archived)","RXF42F5V1B (Archived)","RXF50F5V1B (Archived)"]
["Afmetingen","Unit","","Hoogte","mm","556","556","556","556","610"]
["","","","Breedte","mm","740","740","740","740","923"]
["","","","Diepte","mm","343","343","343","343","367"]
["Gewicht","Unit","","","kg","24.0","24.0","24.0","28.0","40.0"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor"]
["Werkingsbereik","Koelen","","Min.","°CDB","-10","-10","-10","-10","-10"]
["","","","Max.","°CDB","48","48","48","48","48"]
["","Verwarmen","","Min.","°CWB","-15","-15","-15","-15","-15"]
["","","","Max.","°CWB","18","18","18","18","18"]
["Geluidsdrukniveau op 1 m","Koelen","","Hoog","dB(A)","46.0","46.0","48.0","48.0","48.0"]
["","Verwarmen","","Hoog","dB(A)","47.0","47.0","48.0","48.0","49.0"]
["Koelmiddel","Type","","","","R-32","R-32","R-32","R-32","R-32"]
["","Vulling","","","kg","0.420","0.420","0.500","0.750","0.800"]
["Koudemiddel","Vulling","","","tCO2Eq","0.280","0.280","0.340","0.510","0.540"]
["Koelmiddel","GWP","","","","675.0","675.0","675.0","675.0","675.0"]
["Koelleidingmaten","Leidinglengte","","Max.","m","20","20","20","20","30"]
["Leidingaansluitingen","Bijkomende koelmiddelvulling","","","kg/m","002 (voor leidinglengte van meer dan 10 m)","002 (voor leidinglengte van meer dan 10 m)","002 (voor leidinglengte van meer dan 10 m)","002 (voor leidinglengte van meer dan 10 m)","002 (voor leidinglengte van meer dan 10 m)"]
["Koelleidingmaten","Hoogteverschil","","Max.","m","12.0","12.0","12.0","12.0","20.0"]
["Standaard-accessoires","Installation manual","","","","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1"]
["","General safety precautions","","","","1","1","1","1"]
["","Drain plug","","","","1","1","1","1"]
["Voeding","Fase","","","","1~","1~","1~","1~","1~"]
["Spanningsvorm","Frequentie","","","Hz","50","50","50","50","50"]
["","Spanning","","","V","220-240","220-240","220-240","220-240","220-240"]
["Opmerkingen","","","","","(1) - Bevat gefluoreerde broeikasgassen","(1) - Bevat gefluoreerde broeikasgassen","(1) - Bevat gefluoreerde broeikasgassen","(1) - Bevat gefluoreerde broeikasgassen","(1) - Bevat gefluoreerde broeikasgassen"]
["","","","","","(2) - Voor elektrische gegevens zie afzonderlijke tekening","(2) - Voor elektrische gegevens zie afzonderlijke tekening","(2) - Voor elektrische gegevens zie afzonderlijke tekening","(2) - Voor elektrische gegevens zie afzonderlijke tekening","(2) - Voor elektrische gegevens zie afzonderlijke tekening"]
["","","","","","(3) - Zie afzonderlijke afbeelding voor bedrijfsbereik","(3) - Zie afzonderlijke afbeelding voor bedrijfsbereik","(3) - Zie afzonderlijke afbeelding voor bedrijfsbereik","(3) - Zie afzonderlijke afbeelding voor bedrijfsbereik","(3) - Zie afzonderlijke afbeelding voor bedrijfsbereik"]