{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXM-A8"]
[]
[]
[]
[]
["","","","","","RXM50A5V1B8 (Archived)"]
["Afmetingen","Unit","","Hoogte","mm","610"]
["","","","Breedte","mm","923"]
["","","","Diepte","mm","367"]
["Gewicht","Unit","","","kg","40"]
["Ventilatormotor","Snelheid","Koelen","Superlaag","rpm","600"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor"]
["Werkingsbereik","Koelen","","Min.","°C DB","-10"]
["","","","Max.","°C DB","50, 46"]
["","Verwarmen","","Min.","°CWB","-21 (1), -15 (1)"]
["","","","Max.","°CWB","18"]
["Geluidsdrukniveau op 1 m","Koelen","","Nom.","dB(A)","48"]
["","Verwarmen","","Nom.","dB(A)","49"]
["Koelmiddel","Type","","","","R-32"]
["","Vulling","","","kg","0.95"]
["Koudemiddel","Vulling","","","tCO2Eq","0.65"]
["Koelmiddel","GWP","","","","675"]
["Koelleidingmaten","Leidinglengte","","Max.","m","30"]
["Leidingaansluitingen","Bijkomende koelmiddelvulling","","","kg/m","002"]
["Koelleidingmaten","Hoogteverschil","","Max.","m","20"]
["Standaard-accessoires","Installation manual","","","","1"]
["","Drain joint","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","General safety precautions","","","","1"]
["","LOT10 Energy Label","","","","1"]
["","Drain cap","","","","3"]
["Voeding","Fase","","","","1~"]
["Spanningsvorm","Frequentie","","","Hz","50"]
["","Spanning","","","V","220-240"]
["Opmerkingen","","","","","(1) - Zie afzonderlijke afbeelding voor bedrijfsbereik"]
["","","","","","(2) - Voor elektrische gegevens zie afzonderlijke tekening"]
["","","","","","(3) - Bevat gefluoreerde broeikasgassen"]