{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":11,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXP-N9"]
[]
[]
[]
[]
["","","","","","RXP20N5V1B9","RXP25N5V1B9","RXP35N5V1B9","RXP50N5V1B9","RXP60N5V1B9","RXP71N5V1B9"]
["Afmetingen","Unit","","Hoogte","mm","556","556","556","734","734","734"]
["","","","Breedte","mm","740","740","740","954","954","954"]
["","","","Diepte","mm","343","343","343","401","401","401"]
["Gewicht","Unit","","","kg","24","24","26","46","50","50"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor"]
["Werkingsbereik","Koelen","","Min.","°C DB","-10","-10","-10","-10","-10","-10"]
["","","","Max.","°C DB","48","48","48","48","48","48"]
["","Verwarmen","","Min.","°CWB","-15","-15","-15","-15","-15","-15"]
["","","","Max.","°CWB","18","18","18","18","18","18"]
["Geluidsdrukniveau op 1 m","Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Hoog-=-dB(A)","dB(A)","46","46","48"]
["","","","Nom.","dB(A)","","","","47","49","52"]
["","Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Hoog-=-dB(A)","dB(A)","47","47","48"]
["","","","Nom.","dB(A)","","","","49","49","52"]
["Koelmiddel","Type","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Vulling","","","kg","0.55","0.55","0.70","0.9","1.15","1.15"]
["Koudemiddel","Vulling","","","tCO2Eq","0.37","0.37","0.48","0.61","0.78","0.78"]
["Koelmiddel","GWP","","","","675.0","675.0","675.0","675","675","675"]
["Koelleidingmaten","Leidinglengte","","Max.","m","20","20","20","30","30","30"]
["Leidingaansluitingen","Bijkomende koelmiddelvulling","","","kg/m","0,02 (voor leidinglengte van meer dan 10 m)","0,02 (voor leidinglengte van meer dan 10 m)","0,02 (voor leidinglengte van meer dan 10 m)","0,02 (voor leidinglengte van meer dan 10 m)","0,02 (voor leidinglengte van meer dan 10 m)","0,02 (voor leidinglengte van meer dan 10 m)"]
["Koelleidingmaten","Hoogteverschil","","Max.","m","12","12","12","20","20","20"]
["Standaard-accessoires","Installation manual","","","","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","Drain plug","","","","1","1","1","1","1","1"]
["Voeding","Fase","","","","1~","1~","1~","1~","1~","1~"]
["Spanningsvorm","Frequentie","","","Hz","50","50","50","50","50","50"]
["","Spanning","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Standaard-accessoires","Drain cap","","","","","","","3","3","3"]
["Opmerkingen","","","","","","","","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range"]
["","","","","","","","","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data"]
["","","","","","","","","(3) - Bevat gefluoreerde broeikasgassen","(3) - Bevat gefluoreerde broeikasgassen","(3) - Bevat gefluoreerde broeikasgassen"]