{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":59,"n_cols":12,"rows_kept":59,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-K"]
[]
[]
[]
[]
["","","","","","RXS20K3V1B","RXS20K2V1B","RXS25K3V1B","RXS25K2V1B","RXS35K2V1B","RXS42K2V1B","RXS50K2V1B"]
["Geluidsdrukniveau op 1 m","Verwarmen","","Hoog","dB(A)","47","","47","","48","48","48"]
["","Koelen","","Hoog","dB(A)","46","","46","","48","48","48"]
["Standaard-accessoires","Koppeling (afvoer)","","","","1","","1"]
["","Montagehandleiding","","","","1","","1","","1","1","1"]
["Koelmiddel","Charge","","","TCO2Eq","2.1","","2.1","","2.5","2.7","3.5"]
["","GWP","","","","2,087.5","","2,087.5","","2,087.5","2,087.5","2,087.5"]
["","Charge","","","kg","1.0","","1.0","","1.2","1.3","1.7"]
["","Type","","","","R-410A","","R-410A","","R-410A","R-410A","R-410A"]
["Ventilatormotor","Snelheid","Koelen","Superlaag","rpm","780","","780","","780","790","670"]
["","","Verwarmen","Superlaag","rpm","740","","740","","740","780","670"]
["Koelleidingmaten","Hoogteverschil","","Max.","m","15","","15","","15","15","20"]
["","Bijkomende koelmiddelvulling","","","kg/m","0,02 (voor leidinglengte van meer dan 10 m)","","0,02 (voor leidinglengte van meer dan 10 m)","","0,02 (voor leidinglengte van meer dan 10 m)","0,02 (voor leidinglengte van meer dan 10 m)","0,02 (voor leidinglengte van meer dan 10 m)"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor","","Hermetisch gesloten swingcompressor","","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor"]
["Afmetingen","Unit","","Breedte","mm","765","","765","","765","765","825"]
["","","","Diepte","mm","285","","285","","285","285","300"]
["","","","Hoogte","mm","550","","550","","550","550","735"]
["Gewicht","Unit","","","kg","34","","34","","34","39","47"]
["Ventilator","Luchthoeveelheid","Verwarmen","Superlaag","cfm","","","","","904","960","1,522"]
["","","Koelen","Superlaag","cfm","","","","","1,063","1,080","1,727"]
["Power supply","Fase","","","","1~","","1~","","1~","1~","1~"]
["","Frequentie","","","Hz","50","","50","","50","50","50"]
["","Spanning","","","V","220-240","","220-240","","220-240","220-240","220-240"]
["Opmerkingen","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","(4) - SL: de geluidsarme instelling van de ventilator van de luchtcirculatie","","(4) - SL: de geluidsarme instelling van de ventilator van de luchtcirculatie","","(4) - Bevat gefluoreerde broeikasgassen","(4) - Bevat gefluoreerde broeikasgassen","(4) - Bevat gefluoreerde broeikasgassen"]
["","","","","","(5) - Bevat gefluoreerde broeikasgassen","","(5) - Bevat gefluoreerde broeikasgassen"]
["Afmetingen","Unit","","Hoogte","mm","","550","","550"]
["","","","Breedte","mm","","765","","765"]
["","","","Diepte","mm","","285","","285"]
["Gewicht","Unit","","","kg","","34","","34"]
["Ventilatormotor","Snelheid","Koelen","Superlaag","rpm","","780","","780"]
["","","Verwarmen","Superlaag","rpm","","740","","740"]
["Compressor","Type","","","","","Hermetisch gesloten swingcompressor","","Hermetisch gesloten swingcompressor"]
["Werkingsbereik","Koelen","","Min.","°CDB","","-10","","-10"]
["","","","Max.","°CDB","","46","","46"]
["","Verwarmen","","Min.","°CWB","","-15","","-15"]
["","","","Max.","°CWB","","18","","18"]
["Geluidsdrukniveau op 1 m","Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Hoog-=-dB(A)","dB(A)","","46","","46"]
["","Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Hoog-=-dB(A)","dB(A)","","47","","47"]
["Koelmiddel","Type","","","","","R-410A","","R-410A"]
["","Vulling","","","kg","","1.0","","1.0"]
["Koudemiddel","Vulling","","","tCO2Eq","","2.1","","2.1"]
["Koelmiddel","GWP","","","","","2087.5","","2087.5"]
["Koelleidingmaten","Leidinglengte","","Max.","m","","20","","20"]
["Leidingaansluitingen","Bijkomende koelmiddelvulling","","","kg/m","","0,02 (voor leidinglengte van meer dan 10 m)","","0,02 (voor leidinglengte van meer dan 10 m)"]
["Koelleidingmaten","Hoogteverschil","","Max.","m","","15","","15"]
["Standaard-accessoires","Installation manual","","","","","1","","1"]
["","Joint (drain)","","","","","1","","1"]
["Voeding","Fase","","","","","1~","","1~"]
["Spanningsvorm","Frequentie","","","Hz","","50","","50"]
["","Spanning","","","V","","220-240","","220-240"]
["Standaard-accessoires","Aftapplug","","","","","","","","1","1","1"]