{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":13,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-NY1"]
[]
[]
[]
[]
["","","","","","RZAG71N2Y1B","RZAG71N7Y1B","RZAG100N7Y1B","RZAG100N2Y1B","RZAG125N7Y1B","RZAG125N2Y1B","RZAG140N7Y1B","RZAG140N2Y1B"]
["Afmetingen","Unit","","Hoogte","mm","870","870","870","870","870","870","870","870"]
["","","","Breedte","mm","1100","1100","1100","1100","1100","1100","1100","1100"]
["","","","Diepte","mm","460","460","460","460","460","460","460","460"]
["Gewicht","Unit","","","kg","81","81","85","85","94","94","94","94"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor"]
["Werkingsbereik","Koelen","","Min.","°C DB","-20","-20","-20","-20","-20","-20","-20","-20"]
["","","","Max.","°C DB","52","52","52","52","52","52","52","52"]
["","Verwarmen","","Min.","°CWB","-20","-20","-20","-20","-20","-20","-20","-20"]
["","","","Max.","°CWB","18","18","18","18","18","18","18","18"]
["Geluidsvermogenniveau","Koelen","","","dB(A)","64","64","66","66","69","69","70","70"]
["","Verwarmen","","","dB(A)","","","","","68 (1)","68 (1)","71 (1)","71 (1)"]
["Geluidsdrukniveau op 1 m","Koelen","","Nom.","dB(A)","46","46","47","47","49","49","50","50"]
["","Verwarmen","","Nom.","dB(A)","48","48","50","50","52","52","52","52"]
["Koelmiddel","Type","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Vulling","","","kg","3.20","3.2","3.2","3.20","3.7","3.70","3.7","3.70"]
["","GWP","","","","675","675","675","675","675","675","675","675"]
["Koudemiddel","Vulling","","","tCO2Eq","2.16","2.16","2.16","2.16","2.5","2.50","2.5","2.50"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","10","10","10","10","10","10","10","10"]
["","Gas","","Buitendiameter","mm","15.9","15.9","15.9","15.9","15.9","15.9","15.9","15.9"]
["Koelleidingmaten","Leidinglengte","","Max.","m","55","55","85","85","85","85","85","85"]
["","","Systeem","Equivalent","m","75","75","100","100","100","100","100","100"]
["","","Voorgevuld tot","","m","40","40","40","40","40","40","40","40"]
["Leidingaansluitingen","Bijkomende koelmiddelvulling","","","kg/m","Zie installatiehandleiding","Zie installatiehandleiding","Zie installatiehandleiding","Zie installatiehandleiding","Zie installatiehandleiding","Zie installatiehandleiding","Zie installatiehandleiding","Zie installatiehandleiding"]
["Koelleidingmaten","Hoogteverschil","","Max.","m","30","30","30","30","30","30","30","30"]
["","","IU - IU","Max.","m","0.5","0.5","0.5","0.5","0.5","0.5","0.5","0.5"]
["Standaard-accessoires","Installation manual","","","","1","1","1","1","1","1","1","1"]
["","Refrigerant label for F-gas regulation","","","","1","1","1","1","1","1","1","1"]
["","General safety precautions","","","","1","1","1","1","1","1","1","1"]
["","Peel off F-gas label","","","","1","1","1","1","1","1","1","1"]
["","Tie-wraps","","","","2","2","2","2","2","2","2","2"]
["Voeding","Fase","","","","3~","3~","3~","3~","3~","3~","3~","3~"]
["Spanningsvorm","Frequentie","","","Hz","50","50","50","50","50","50","50","50"]
["","Spanning","","","V","380-415","380-415","380-415","380-415","380-415","380-415","380-415","380-415"]
["Stroom: 50 Hz","Maximaal zekeringamperage (MFA)","","","A","16","16","16","16","16","16","16","16"]
["Opmerkingen","","","","","","","","","(1) - Volgens ENER Lot 21","(1) - Volgens ENER Lot 21","(1) - Volgens ENER Lot 21","(1) - Volgens ENER Lot 21"]