{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":8,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZASG-MV"]
[]
[]
[]
[]
["","","","","","RZASG100MUV","RZASG125MUV","RZASG140MUV"]
["Afmetingen","Afmetingen-=-Unit","","Afmetingen-=-Unit-=-Hoogte-=-mm","mm","990","990","990"]
["","","","Afmetingen-=-Unit-=-Breedte-=-mm","mm","940","940","940"]
["","","","Afmetingen-=-Unit-=-Diepte-=-mm","mm","320","320","320"]
["Gewicht","Gewicht-=-Unit-=-kg","","","kg","72","72","79"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor"]
["Werkingsbereik","Werkingsbereik-=-Koelen","Werkingsbereik-=-Koelen-=- ","Werkingsbereik-=-Koelen-=- -=-Min.-=-°CDB","°C DB","-15","-15","-15"]
["","","","Werkingsbereik-=-Koelen-=- -=-Max.-=-°CDB","°C DB","46","46","46"]
["","Werkingsbereik-=-Verwarmen","Werkingsbereik-=-Verwarmen-=- ","Werkingsbereik-=-Verwarmen-=- -=-Min.-=-°CWB","°CWB","-15","-15","-15"]
["","","","Werkingsbereik-=-Verwarmen-=- -=-Max.-=-°CWB","°CWB","15.5","15.5","15.5"]
["Geluidsvermogenniveau","Geluidsvermogenniveau-=-Koelen-=-dBA","","","dB(A)","70","71","73"]
["","Geluidsvermogenniveau-=-Verwarmen-=-dBA","","","dB(A)","","71 (1)","73 (1)"]
["Geluidsdrukniveau op 1 m","Geluidsdrukniveau op 1 m-=-Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Nom.-=-dBA","dB(A)","53","53","54"]
["","Geluidsdrukniveau op 1 m-=-Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Nom.-=-dBA","dB(A)","57","57","57"]
["Koelmiddel","Koelmiddel-=-Type","","","","R-32","R-32","R-32"]
["","Koelmiddel-=-Vulling-=-kg","","","kg","2.6","2.6","2.9"]
["","Koelmiddel-=-GWP","","","","675","675","675"]
["Koudemiddel","Koudemiddel-=-Vulling-=-tCO2eq","","","tCO2Eq","1.76","1.76","1.96"]
["Leidingaansluitingen","Leidingaansluitingen-=-Vloeistof","","Leidingaansluitingen-=-Vloeistof-=-Buitendiameter-=-mm","mm","9.52","9.52","9.52"]
["","Leidingaansluitingen-=-Gas","","Leidingaansluitingen-=-Gas-=-Buitendiameter-=-mm","mm","15.9","15.9","15.9"]
["Koelleidingmaten","Koelleidingmaten-=-Leidinglengte","Koelleidingmaten-=-Leidinglengte-=- ","Koelleidingmaten-=-Leidinglengte-=- -=-Max.-=-m","m","50","50","50"]
["","","Koelleidingmaten-=-Leidinglengte-=-Systeem","Koelleidingmaten-=-Leidinglengte-=-Systeem-=-Equivalent-=-m","m","70","70","70"]
["","","Koelleidingmaten-=-Leidinglengte-=-Voorgevuld tot","Koelleidingmaten-=-Leidinglengte-=-Voorgevuld tot-=- -=-m","m","30","30","30"]
["Leidingaansluitingen","Leidingaansluitingen-=-Bijkomende koelmiddelvulling-=-kg/m","","","kg/m","Zie installatiehandleiding","Zie installatiehandleiding","Zie installatiehandleiding"]
["Koelleidingmaten","Koelleidingmaten-=-Hoogteverschil","Koelleidingmaten-=-Hoogteverschil-=- ","Koelleidingmaten-=-Hoogteverschil-=- -=-Max.-=-m","m","30","30","30"]
["","","Koelleidingmaten-=-Hoogteverschil-=-IU - IU","Koelleidingmaten-=-Hoogteverschil-=-IU - IU-=-Max.-=-m","m","0.5","0.5","0.5"]
["Standaard-accessoires","Installation manual","","","","1","1","1"]
["","Refrigerant label for F-gas regulation","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1"]
["","Declaration of conformity","","","","2","2","2"]
["","Tie-wraps","","","","2","2","2"]
["Voeding","Voeding-=-Fase","","","","1~","1~","1~"]
["Spanningsvorm","Spanningsvorm-=-Frequentie-=-Hz","","","Hz","50","50","50"]
["","Spanningsvorm-=-Spanning-=-V","","","V","220-240","220-240","220-240"]
["Stroom: 50 Hz","Stroom: 50 Hz-=-Maximaal zekeringamperage (MFA)-=-A","","","A","25","32","32"]
["Opmerkingen","","","","","(1) - Volgens ENER Lot 21","(1) - Volgens ENER Lot 21","(1) - Volgens ENER Lot 21"]
["","","","","","(2) - European/international technical standard setting the limits for harmonic currents produced by equipment connected to public low-voltage system with input current larger than 16A and ≤ 75A per phase.","(2) - European/international technical standard setting the limits for harmonic currents produced by equipment connected to public low-voltage system with input current larger than 16A and ≤ 75A per phase.","(2) - European/international technical standard setting the limits for harmonic currents produced by equipment connected to public low-voltage system with input current larger than 16A and ≤ 75A per phase."]
["","","","","","(3) - Ssc: kortsluitvermogen","(3) - Ssc: kortsluitvermogen","(3) - Ssc: kortsluitvermogen"]
["","","","","","(4) - Europese/internationale technische norm die de grenswaarden bepaalt voor harmonische stromen, gegenereerd door apparatuur die wordt aangesloten op een openbaar laagspanningssysteem met ingangsstroom ≤ 16A per fase.","","(4) - Europese/internationale technische norm die de grenswaarden bepaalt voor harmonische stromen, gegenereerd door apparatuur die wordt aangesloten op een openbaar laagspanningssysteem met ingangsstroom ≤ 16A per fase."]