{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2AMXF-A"]
[]
[]
[]
[]
["","","","","","2AMXF40A2V1B"]
["Afmetingen","Unit","","Hoogte","mm","550"]
["","","","Breedte","mm","765"]
["","","","Diepte","mm","285"]
["Gewicht","Unit","","","kg","36"]
["Ventilatormotor","Snelheid","Koelen","Superlaag","rpm","500"]
["","","Verwarmen","Superlaag","rpm","320"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor"]
["Werkingsbereik","Koelen","","Min.","°CDB","-10"]
["","","","Max.","°CDB","46"]
["Geluidsdrukniveau op 1 m","Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Hoog-=-dB(A)","dBA","46"]
["","Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Hoog-=-dB(A)","dBA","48"]
["Koelmiddel","Type","","","","R-32"]
["","Vulling","","","kg","0.88"]
["Koudemiddel","Vulling","","","tCO2Eq","0.60"]
["Koelmiddel","GWP","","","","675"]
["Koelleidingmaten","Leidinglengte","","Max.","m","20"]
["Leidingaansluitingen","Bijkomende koelmiddelvulling","","","kg/m","0,02 (voor leidinglengte van meer dan 20 m)"]
["Koelleidingmaten","Hoogteverschil","","Max.","m","15.0"]
["","","IU - IU","Max.","m","7.5"]
["","Totale leidinglengte","Systeem","Werkelijk","m","30"]
["Standaard-accessoires","Installation manual","","","","1"]
["","Drain plug","","","","1"]
["","Screw bag","","","","1"]
["Voeding","Fase","","","","1~"]
["Spanningsvorm","Frequentie","","","Hz","50"]
["","Spanning","","","V","220-230-240"]
["Opmerkingen","","","","","(1) - Van één kamer"]