{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":9,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-N"]
[]
[]
[]
[]
["","","","","","ATXM20N2V1B","ATXM25N2V1B","ATXM35N2V1B","ATXM50N2V1B"]
["Opgenomen vermogen","Koelen","","Nom.","kW","0.03","0.03","0.034","0.03"]
["","Verwarmen","","Nom.","kW","0.025","0.026","0.026","0.032"]
["Behuizing","Kleur","","","","Wit","Wit","Wit","Wit"]
["Afmetingen","Unit","","Hoogte","mm","294","294","294","300"]
["","","","Breedte","mm","811","811","811","1040"]
["","","","Diepte","mm","272","272","272","295"]
["Gewicht","Unit","","","kg","10","10","10","14.5"]
["Ventilator-","Luchthoeveelheid","Koelen","Hoog","m³/min","11.1","11.1","12.3","16.1"]
["Ventilator","Luchtdebiet","Koeling","Middelhoog","m³/min","7.9","8.1","8.3","14.2"]
["Ventilator-","Luchthoeveelheid","Koelen","Laag","m³/min","6","6.2","6.4","11.6"]
["","","","Fluisterstille werking","m³/min","4.4","4.4","4.6","8.1"]
["","","Verwarmen","Hoog","m³/min","10.8","10.8","10.8","17.1"]
["Ventilator","Luchtdebiet","Verwarming","Middelhoog","m³/min","8.7","8.7","9","14.6"]
["Ventilator-","Luchthoeveelheid","Verwarmen","Laag","m³/min","6.5","6.8","7.1","12.2"]
["","","","Fluisterstille werking","m³/min","5.3","5.3","5.3","10.7"]
["Geluidsvermogenniveau","Koelen","","","dB(A)","58","58","58","58"]
["","Verwarmen","","","dB(A)","55","55","55","58"]
["Geluidsdrukniveau op 1 m","Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Hoog-=-dB(A)","dB(A)","41","41","45","44"]
["Geluidsdrukniveau","Koeling","","Middelhoog","dB(A)","33","33","33","40"]
["Geluidsdrukniveau op 1 m","Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Laag-=-dB(A)","dB(A)","25","25","29","36"]
["","","","Geluidsdrukniveau op 1 m-=-Koelen-=-Fluisterstille werking-=-dB(A)","dB(A)","19","19","19","27"]
["","Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Hoog-=-dB(A)","dB(A)","39","39","39","43"]
["Geluidsdrukniveau","Verwarming","","Middelhoog","dB(A)","34","34","35","39"]
["Geluidsdrukniveau op 1 m","Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Laag-=-dB(A)","dB(A)","26","27","28","34"]
["","","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Fluisterstille werking-=-dB(A)","dB(A)","20","20","20","31"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","6.35","6.35","6.35","6.35"]
["","Gas","","Buitendiameter","mm","9.5","9.5","9.5","12.7"]
["","Drainage","","","","18","18","18","18"]
["Regelsystemen","Infrared remote control","","","","ARC466A33","ARC466A33","ARC466A33","ARC466A33"]
["Regelsystemen","Bedrade afstandsbediening","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Standaard-accessoires","Installation manual","","","","1","1","1","1"]
["","Wireless remote control","","","","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2"]
["","WLAN adapter kit","","","","1","1","1","1"]
["","Operation manual","","","","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1","1","2"]
["","Indoor unit fixing screws","","","","2","2","2","2"]
["","Mounting plate","","","","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1"]
["Voeding","Naam","","","","V1","V1","V1","V1"]
["","Fase","","","","1~","1~","1~","1~"]
["Spanningsvorm","Frequentie","","","Hz","50","50","50","50"]
["","Spanning","","","V","220-240","220-240","220-240","220-240"]