{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":7,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BPMKS967A"]
[]
[]
[]
[]
["","","","","","BPMKS967B2B","BPMKS967B3B"]
["Standaard-accessoires","Montagehandleiding","","","","1","1"]
["","Verloopstuk voor kant buitenunit; Gasdiameter 12,7","","","","1","1"]
["","Verloopstuk voor kant buitenunit; Gasdiameter 15,9","","","","1","1"]
["","Verloopstuk voor kant buitenunit; Gasdiameter 19,1","","","","1","1"]
["","Verloopstuk voor kant buitenunit; Vloeistofdiameter 6,4","","","","1","1"]
["","Verloopstuk voor kant binnenunit; Gasdiameter 9.52","","","","1","1"]
["","Verloopstuk voor kant binnenunit; Vloeistofdiameter 12,7","","","","2","3"]
["","Verloopstuk voor kant binnenunit; Vloeistofdiameter 9,5","","","","2","3"]
["","Ophangbeugel","","","","4","4"]
["","Schroeven (M4x8)","","","","8","8"]
["","Thermische isolatie","","","","3","4"]
["","Bundelband","","","","2","2"]
["Afmetingen","Unit","","Breedte","mm","650","650"]
["","","","Diepte","mm","350","350"]
["","","","Hoogte","mm","180","180"]
["Gewicht","Unit","","","kg","7.5","8"]
["Aansluitbaar type binnendeel","","","","","Bouwgrootte 20 - 71","Bouwgrootte 20 - 71"]
["Koelleidingmaten","Buitendeel","Vloeistof","Aantal","","1","1"]
["","","","ID","mm","9.5","9.5"]
["","","Gas","Aantal","mm","1","1"]
["","","","ID","mm","19.1","19.1"]
["","Binnendeel","Gas","Aantal","mm","2","3"]
["","","","ID","mm","15.9","15.9"]
["","","Vloeistof","ID","mm","6.4","6.4"]
["","","","Aantal","","2","3"]
["","Afvoer","","ID","mm","Afvoer zonder verwerking","Afvoer zonder verwerking"]
["Opgenomen vermogen","Nom.","","","kW","0.010","0.010"]
["Power supply","Frequentie","","","Hz","50","50"]
["","Spanning","","","V","230","230"]