{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":7,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-R"]
[]
[]
[]
[]
["","","","","","CTXM15R2V1B","CTXM15R5V1B"]
["Opgenomen vermogen","Koelen","","Nom.","kW","0.029","0.029"]
["","Verwarmen","","Nom.","kW","0.023","0.023"]
["Behuizing","Kleur","","","","Wit","Wit"]
["Afmetingen","Unit","","Hoogte","mm","295","295"]
["","","","Breedte","mm","778","778"]
["","","","Diepte","mm","272","272"]
["Gewicht","Unit","","","kg","10","10"]
["Ventilator-","Luchthoeveelheid","Koelen","Hoog","m³/min","10.5","10.5"]
["Ventilator","Luchtdebiet","Koeling","Middelhoog","m³/min","7.5","7.5"]
["Ventilator-","Luchthoeveelheid","Koelen","Laag","m³/min","5.7","5.7"]
["","","","Fluisterstille werking","m³/min","4.3","4.3"]
["","","Verwarmen","Hoog","m³/min","9.3","9.3"]
["Ventilator","Luchtdebiet","Verwarming","Middelhoog","m³/min","8.2","8.2"]
["Ventilator-","Luchthoeveelheid","Verwarmen","Laag","m³/min","6.2","6.2"]
["","","","Fluisterstille werking","m³/min","5.1","5.1"]
["Geluidsvermogenniveau","Koelen","","","dB(A)","57","57"]
["","Verwarmen","","","dB(A)","54","54"]
["Geluidsdrukniveau op 1 m","Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Hoog-=-dB(A)","dB(A)","41","41"]
["Geluidsdrukniveau","Koeling","","Middelhoog","dB(A)","33","33"]
["Geluidsdrukniveau op 1 m","Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Laag-=-dB(A)","dB(A)","25","25"]
["","","","Geluidsdrukniveau op 1 m-=-Koelen-=-Fluisterstille werking-=-dB(A)","dB(A)","19","19"]
["","Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Hoog-=-dB(A)","dB(A)","39","39"]
["Geluidsdrukniveau","Verwarming","","Middelhoog","dB(A)","34","34"]
["Geluidsdrukniveau op 1 m","Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Laag-=-dB(A)","dB(A)","26","26"]
["","","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Fluisterstille werking-=-dB(A)","dB(A)","20","20"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","6.35","6.35"]
["","Gas","","Buitendiameter","mm","9.5","9.5"]
["","Drainage","","","","18","18"]
["Regelsystemen","Infrared remote control","","","","ARC466A67","ARC466A67"]
["Regelsystemen","Bedrade afstandsbediening","","","","BRC073A1","BRC073A1"]
["Standaard-accessoires","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","WLAN adapter kit","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Indoor unit fixing screws","","","","2","2"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["Voeding","Naam","","","","V1","V1"]
["","Fase","","","","1~","1~"]
["Spanningsvorm","Frequentie","","","Hz","50","50"]
["","Spanning","","","V","220-240","220-240"]