{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DCS601C51"]
[]
[]
[]
[]
["","","","","","DCS601C51."]
["Ingang","Type","","","","Aanraakscherm (10 bit gecodeerd analoge input)"]
["Omgevingstemperatuur","Relatieve vochtigheid <","","","%","85"]
["","Bedrijf","","Min.","°C","0"]
["","","","Max.","°C","40"]
["Maximaal aantal aansluitbare binnendelen","","","","","64, 128 (1)"]
["Communicatie","DIII-NET","","Aantal","","1"]
["","","","Opmerking","","Communicatielijn airconditioning"]
["","10BASE-T","","Opmerking","","Web optie"]
["","Ethernet","","Opmerking","","Poort voor internettoegang en e-mailfunctie"]
["","Ingangsklem","Digitaal","Aantal","","1"]
["","","","Opmerking","","Geforceerde uitschakeling"]
["","","Puls","Aantal","","3"]
["","","","Opmerking","","Stroommeetpuls"]
["","Modem","","Opmerking","","Onboard-modem mogelijk"]
["","PCMCIA","","Opmerking","","Flash-geheugenkaart"]
["","RS-232C","","Opmerking","","DIII-NET plus adapter"]
["Afmetingen","Unit","","Breedte","mm","230"]
["","","","Diepte","mm","107"]
["","","","Hoogte","mm","147"]
["LCD","Type","","","","QVGA (320 x 240), 4.096 kleuren"]
["","Afmetingen","","B","inch","5.7"]
["Maximaal aantal aansluitbare buitendelen","","","","","10, 20 (1)"]
["Power supply","Frequentie","","","Hz","50/60"]
["","Spanning","","","V","100-240 (extern voorzien)"]
["Opmerkingen","","","","","(1) - In combinatie met DCS601A51"]