{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DMS504B51"]
[]
[]
[]
[]
["","","","","","DMS504B51."]
["Omgevingstemperatuur","Relatieve vochtigheid <","","","%","95"]
["","Bewaring","","Min.","°C","-20"]
["","","","Max.","°C","60"]
["","Bedrijf","","Min.","°C","-10"]
["","","","Max.","°C","50"]
["Communicatie","Ingangsklem","Digitaal","Aantal","","1"]
["","","","Opmerking","","Geforceerde uitschakeling"]
["","Overdracht","","Middelhoog","","Twisted pair kabel"]
["","","","Snelheid","Kbps","78"]
["Montage","","","","","Gemonteerd op interne verdeelkast"]
["Afmetingen","Unit","","Breedte","mm","168"]
["","","","Diepte","mm","50"]
["","","","Hoogte","mm","260"]
["Topologie","","","","","FTT-10A (Vrije topologie)"]
["Gewicht","Unit","","","kg","1.5"]
["Power supply","Fase","","","","1~"]
["","Frequentie","","","Hz","50/60"]
["","Spanning","","","V","AC 100-240"]