{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":6,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EBLA-D3W17"]
[]
[]
[]
[]
["","","","","","EBLA16DA3W17"]
["Totale verwarmingscapaciteit","Nom.","","","kW","16.0 (1) (2)"]
["Totale koelcapaciteit","Nom.","","","kW","14.0 (3), 15.3 (4)"]
["Capaciteit verwarmer","Stap 1","","","kW","3"]
["Opgenomen vermogen","Koelen","","Nom.","kW","4.58 (3), 3.24 (4)"]
["","Verwarmen","","Nom.","kW","3.53 (1), 4.56 (2)"]
["COP","","","","","4.53 (1), 3.51 (2)"]
["EER","","","","","3.06 (3), 4.74 (4)"]
["Afmetingen","Unit","","Hoogte","mm","870"]
["","","","Breedte","mm","1380"]
["","","","Diepte","mm","460"]
["Gewicht","Unit","","","kg","149"]
["Ventilator-","Luchthoeveelheid","Verwarmen","Hoog","m³/min","85.0"]
["","","Koelen","Hoog","m³/min","85.0"]
["Werkingsbereik","Verwarmen","waterzijdig","Min.","°C","15 (6)"]
["","","","Max.","°C","60 (6)"]
["","Koelen","","Min.","°CDB","10"]
["","","","Max.","°CDB","43"]
["","","Waterzijde","Min.","°C","5"]
["","","","Max.","°C","22"]
["","Warmtapwater","Omgeving","Min.","°CDB","-25"]
["","","","Max.","°CDB","35"]
["","","Waterzijde","Min.","°C","25"]
["","","","Max.","°C","55 (6)"]
["Koelmiddel","Type","","","","R-32"]
["","GWP","","","","675"]
["","Vulling","","","kg","3.80"]
["Koudemiddel","Vulling","","","tCO2Eq","2.57"]
["Verwarming","Wateruitlaat gematigd klimaat 55°C","Algemeen","SCOP","","3.37"]
["","","","Seizoensefficiëntieklasse verwarming","","A++"]
["","Wateruitlaat gematigd klimaat 35°C","Algemeen","SCOP","","4.69"]
["","","","Seizoensefficiëntieklasse verwarming","","A+++"]
["Bereik van het energierendement","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Compressorcomponent","Netvoeding","","Fase","","3N~"]
["","","","Spanning","V","400"]
["Voeding","Naam","","","","W1"]
["","Fase","","","","3~"]
["Spanningsvorm","Frequentie","","","Hz","50"]
["","Spanning","","","V","400"]
["Opmerkingen","","","","","(1) - Voorwaarde: Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Voorwaarde: Ta DB/WB 7 °C / 6 °C - LWC 45 °C (Dt=5 °C)"]
["","","","","","(3) - Koelen: EW 12°C; LW 7°C; omgevingsomstandigheden: 35°CDB"]
["","","","","","(4) - Koelen: EW 23°C; LW 18°C; omgevingsomstandigheden: 35°CDB"]
["","","","","","(5) - Overeenkomstig EN14825"]
["","","","","","(6) - Raadpleeg de werkbereik-tekening voor meer informatie"]
["","","","","","(7) - Afhankelijk van de bedrijfsmodus, zie installatiehandleiding"]