{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":7,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EDLA09-14DV3"]
[]
[]
[]
[]
["","","","","","EDLA11DAV3 (Archived)","EDLA14DAV3 (Archived)"]
["Totale verwarmingscapaciteit","Nom.","","","kW","10.6 (1), 9.82 (2)","12.0 (1), 12.5 (2)"]
["Opgenomen vermogen","Verwarmen","","Nom.","kW","2.18 (1), 2.68 (2)","2.46 (1), 3.42 (2)"]
["COP","","","","","4.83 (1), 3.66 (2)","4.87 (1), 3.64 (2)"]
["Afmetingen","Unit","","Hoogte","mm","870","870"]
["","","","Breedte","mm","1380","1380"]
["","","","Diepte","mm","460","460"]
["Gewicht","Unit","","","kg","147","147"]
["Ventilator-","Luchthoeveelheid","Verwarmen","Hoog","m³/min","55.8","70.4"]
["Werkingsbereik","Verwarmen","waterzijdig","Min.","°C","9 (6)","9 (6)"]
["","","","Max.","°C","60 (6)","60 (6)"]
["","Warmtapwater","Omgeving","Min.","°C DB","-25","-25"]
["","","","Max.","°C DB","35","35"]
["","","Waterzijde","Min.","°C","25","25"]
["","","","Max.","°C","55 (6)","55 (6)"]
["Koelmiddel","Type","","","","R-32","R-32"]
["","GWP","","","","675","675"]
["","Vulling","","","kg","3.80","3.80"]
["Koudemiddel","Vulling","","","tCO2Eq","2.57","2.57"]
["Verwarming","Wateruitlaat gematigd klimaat 55°C","Algemeen","SCOP","","3.32","3.37"]
["","","","Seizoensefficiëntieklasse verwarming","","A++","A++"]
["","Wateruitlaat gematigd klimaat 35°C","Algemeen","SCOP","","4.64","4.62"]
["","","","Seizoensefficiëntieklasse verwarming","","A+++","A+++"]
["Compressorcomponent","Netvoeding","","Fase","","1~","1~"]
["","","","Spanning","V","230","230"]
["Voeding","Naam","","","","V3","V3"]
["","Fase","","","","1~","1~"]
["Spanningsvorm","Frequentie","","","Hz","50","50"]
["","Spanning","","","V","230","230"]
["Opmerkingen","","","","","(1) - Voorwaarde: Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Voorwaarde: Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Voorwaarde: Ta DB/WB 7 °C / 6 °C - LWC 45 °C (Dt=5 °C)","(2) - Voorwaarde: Ta DB/WB 7 °C / 6 °C - LWC 45 °C (Dt=5 °C)"]
["","","","","","(3) - Raadpleeg de werkbereik-tekening voor meer informatie","(3) - Raadpleeg de werkbereik-tekening voor meer informatie"]
["","","","","","(4) - Afhankelijk van de bedrijfsmodus, zie installatiehandleiding","(4) - Afhankelijk van de bedrijfsmodus, zie installatiehandleiding"]