{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKCB-CV3"]
[]
[]
[]
[]
["","","","","EKCB07CAV3"]
["Afmetingen","Unit","Breedte","mm","340"]
["","","Diepte","mm","97.0"]
["","","Hoogte","mm","360"]
["Behuizing","Materiaal","","","Voorgelakte metaalplaat"]
["","Kleur","","","Wit"]
["Gewicht","Unit","","kg","4.00"]
["Bedradingen","Voor voedingsaansluiting van optioneel *KHW* model + Q2L","Opmerking","","Kabeldiameter 2,5 mm2"]
["","","Aantal","","4 + AARDE"]
["","Voor aansluiting met gebruikersinterface","Opmerking","","100 mA, 0,75 mm² tot 1,25 mm² (max. lengte 500 m)"]
["","","Aantal","","2"]
["Power supply","Fase","","","1~"]
["","Frequentie","","Hz","50"]
["","Spanning","","V","230"]
["Spanning","Afzekerwaarde","","A","10"]
["Opmerkingen","","","","(1) - Apparatuur in overeenstemming met EN/IEC 61000-3-12: Europese/internationale technische norm die de grenswaarden bepaalt voor harmonische stromen, gegenereerd door apparatuur die wordt aangesloten op een openbaar laagspanningssysteem met ingangsstroom > 16A and ≤ 75A  per fase"]
["","","","","(2) - Tussen *KCB*C* en *K2CB*C*"]
["","","","","(3) - Selecteer diameter en type conform de nationale en lokale reglementen"]