{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":15,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKEXV"]
[]
[]
[]
[]
["","","","","","EKEXV100","EKEXV125","EKEXV140","EKEXV200","EKEXV250","EKEXV400","EKEXV50","EKEXV500","EKEXV63","EKEXV80"]
["Afmetingen","Unit","","Hoogte","mm","401","401","401","401","401","401","401","401","401","401"]
["","","","Breedte","mm","215","215","215","215","215","215","215","215","215","215"]
["","","","Diepte","mm","78","78","78","78","78","78","78","78","78","78"]
["Gewicht","Unit","","","kg","2.9","2.9","2.9","2.9","2.9","2.9","2.9","2.9","2.9","2.9"]
["Bedrijfsbereik","Koelen","","Min.","°CDB","-5","-5","-5","-5","-5","-5","-5","-5","-5","-5"]
["","","","Max.","°CDB","46","46","46","46","46","46","46","46","46","46"]
["Geluidsdrukniveau op 1 m","Geluidsdrukniveau op 1 m-=-Nom.-=-dB(A)","","","dB(A)","45","45","45","45","45","45","45","45","45","45"]
["Leidingaansluitingen","Vloeistof","","Type","","Hardsoldeerverbinding","Hardsoldeerverbinding","Hardsoldeerverbinding","Hardsoldeerverbinding","Hardsoldeerverbinding","Hardsoldeerverbinding","Hardsoldeerverbinding","Hardsoldeerverbinding","Hardsoldeerverbinding","Hardsoldeerverbinding"]
["","","","Buitendiameter","mm","9.52","9.52","9.52","9.52","9.52","12.70","6.35","15.90","9.52","9.52"]
["","Gas","","Type","","Hardsoldeerverbinding","Hardsoldeerverbinding","Hardsoldeerverbinding","Hardsoldeerverbinding","Hardsoldeerverbinding","Hardsoldeerverbinding","Hardsoldeerverbinding","Hardsoldeerverbinding","Hardsoldeerverbinding","Hardsoldeerverbinding"]
["","","","Buitendiameter","mm","9.52","9.52","9.52","9.52","9.52","9.52","6.35","9.52","9.52","9.52"]
["Koelleidingmaten","Leidinglengte","Voorgevuld tot","","m","0","0","0","0","0","0","0","0","0","0"]
["","Hoogteverschil","IU - IU","Max.","","Zie handleiding, afhankelijk van buitendeel","Zie handleiding, afhankelijk van buitendeel","Zie handleiding, afhankelijk van buitendeel","Zie handleiding, afhankelijk van buitendeel","Zie handleiding, afhankelijk van buitendeel","Zie handleiding, afhankelijk van buitendeel","Zie handleiding, afhankelijk van buitendeel","Zie handleiding, afhankelijk van buitendeel","Zie handleiding, afhankelijk van buitendeel","Zie handleiding, afhankelijk van buitendeel"]
["Opmerkingen","","","","","(2) - Minimum and maximum piping length refer to the piping between the expansion valve kit (EKEXV) and the air handling unit","(2) - Minimum and maximum piping length refer to the piping between the expansion valve kit (EKEXV) and the air handling unit","(2) - Minimum and maximum piping length refer to the piping between the expansion valve kit (EKEXV) and the air handling unit","(2) - Minimum and maximum piping length refer to the piping between the expansion valve kit (EKEXV) and the air handling unit","(2) - Minimum and maximum piping length refer to the piping between the expansion valve kit (EKEXV) and the air handling unit","(2) - Minimum and maximum piping length refer to the piping between the expansion valve kit (EKEXV) and the air handling unit","(2) - Minimum and maximum piping length refer to the piping between the expansion valve kit (EKEXV) and the air handling unit","(2) - Minimum and maximum piping length refer to the piping between the expansion valve kit (EKEXV) and the air handling unit","(2) - Minimum and maximum piping length refer to the piping between the expansion valve kit (EKEXV) and the air handling unit","(2) - Minimum and maximum piping length refer to the piping between the expansion valve kit (EKEXV) and the air handling unit"]